{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXF-A"]
[]
[]
[]
[]
["","","","","","2AMXF40A2V1B"]
["Mere","Enota","","Višina","mm","550"]
["","","","Širina","mm","765"]
["","","","Globina","mm","285"]
["Teža","Enota","","","kg","36"]
["Motor ventilatorja","Hitrost","Hlajenje","Izjwemno nizka","vrt/min","500"]
["","","Ogrevanje","Izjwemno nizka","vrt/min","320"]
["Kompresor","Tip","","","","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","°CDB","-10"]
["","","","Maks.","°CDB","46"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","46"]
["","Gretje","","Visok","dBA","48"]
["Hladilno sredstvo","Tip","","","","R-32"]
["","Polnitev","","","kg","0.88"]
["","Polnjenje","","","tCO2Eq","0.60"]
["","GWP","","","","675"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","20"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 20m)"]
["","Višinska razlika","IU - OU","Maks.","m","15.0"]
["","","IU - IU","Maks.","m","7.5"]
["","Skupna dolžina cevi","Sistem","Dejansko","m","30"]
["Standardni pripomočki","Installation manual","","","","1"]
["","Drain plug","","","","1"]
["","Screw bag","","","","1"]
["Napajanje","Faza","","","","1~"]
["","Frekvenca","","","Hz","50"]
["","Napetost","","","V","220-230-240"]
["Opombe","","","","","(1) - Za en prostor"]