{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-A8"]
[]
[]
[]
[]
["","","","","","2MXM50A2V1B8","2MXM68A2V1B8"]
["Mere","Enota","","Višina","mm","552","734"]
["","","","Širina","mm","852","974"]
["","","","Globina","mm","350","408"]
["Teža","Enota","","","kg","41","60"]
["Kompresor","Tip","","","","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","50","50"]
["Raven zvočnega tlaka","Hlajenje","","Nom.","dBA","48","48"]
["","Gretje","","Nom.","dBA","50","48"]
["Hladilno sredstvo","Tip","","","","R-32","R-32"]
["","Polnitev","","","kg","1.15","2.00"]
["","Polnjenje","","","tCO2Eq","0.78","1.35"]
["","GWP","","","","675","675"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","20 (1)","25 (1)"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 20m)","0,02 (za dolžino napeljave nad 30 m)"]
["","Višinska razlika","IU - OU","Maks.","m","15","15"]
["","","IU - IU","Maks.","m","7.5","7.5"]
["","Skupna dolžina cevi","Sistem","Dejansko","m","30","50"]
["Standardni pripomočki","Priročnik za namestitev","","","","1","1"]
["","Izpustni čep","","","","1","1"]
["","Sklop reduktorja","","","","1","1"]
["","Vrečka vijaka","","","","1","1"]
["Razpon energetske učinkovitosti","","","","","A+++ ~ D","A+++ ~ D"]
["Napajanje","Faza","","","","1~","1~"]
["","Frekvenca","","","Hz","50","50"]
["","Napetost","","","V","220-240","220-240"]
["Opombe","","","","","(1) - Za en prostor","(1) - Za en prostor"]
["","","","","","(2) - Za kombinacijo s CVXM-A, FVXM-A - največja dolžina cevne napeljave je 30 m.","(2) - Za kombinacijo s CVXM-A, FVXM-A - največja dolžina cevne napeljave je 30 m."]
["","","","","","(3) - Glejte ločeno risbo za obratovalno območje","(3) - Glejte ločeno risbo za obratovalno območje"]
["","","","","","(4) - Glejte ločeno risbo za električne podatke","(4) - Glejte ločeno risbo za električne podatke"]
["","","","","","(5) - Vsebuje fluorirane toplogredne pline","(5) - Vsebuje fluorirane toplogredne pline"]
["Standardni pripomočki","Pokrovček izpusta","","","","","3"]