{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-N"]
[]
[]
[]
[]
["","","","","","2MXM40N2V1B","2MXM50N2V1B","2MXM68N2V1B"]
["Mere","Enota","","Višina","mm","550","550","734"]
["","","","Širina","mm","765","765","958"]
["","","","Globina","mm","285","285","340"]
["Teža","Enota","","","kg","36","41","60"]
["Motor ventilatorja","Hitrost","Hlajenje","Izjwemno nizka","obr/min","500","500","420"]
["","","Ogrevanje","Izjwemno nizka","obr/min","320","500","420"]
["Kompresor","Type","","","","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","°CDB","","","-10"]
["","","","Maks.","°CDB","","","46"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","46","48"]
["","","","Nom.","dBA","","","48"]
["","Gretje","","Visok","dBA","48","50"]
["","","","Nom.","dBA","","","48.0"]
["Hladilno sredstvo","Tip","","","","R-32","R-32","R-32"]
["","Polnitev","","","kg","0.88","1.15","2"]
["","Polnjenje","","","tCO2Eq","0.60","0.78","1.35"]
["","GWP","","","","675","675","675.0"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","20","20","25"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 20m)","0,02 (za dolžino napeljave nad 20m)","0,02 (za dolžino napeljave nad 30 m)"]
["","Višinska razlika","IU - OU","Maks.","m","15.0","15.0","15.0"]
["","","IU - IU","Maks.","m","7.5","7.5","7.5"]
["","Skupna dolžina cevi","Sistem","Dejansko","m","30","30","50"]
["Standardni pripomočki","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Napajanje","Faza","","","","1~","1~","1~"]
["","Frekvenca","","","Hz","50","50","50"]
["","Napetost","","","V","220-230-240","220-230-240","220-240"]
["Opombe","","","","","(1) - Za en prostor","(1) - Za en prostor","(1) - Za en prostor"]
["Standardni pripomočki","Reducer assembly","","","","","1","1"]
["","Drain cap","","","","","","3"]