{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXS-H"]
[]
[]
[]
[]
["","","","","","2MXS40H3V1B","2MXS40H3V1B2","2MXS40H2V1B","2MXS50H3V1B2","2MXS50H3V1B","2MXS50H2V1B"]
["Raven zvočnega tlaka","Gretje","","Nom.","dBA","48","48","","50","50"]
["","Hlajenje","","Nom.","dBA","47","47","","48","48"]
["Standardni pripomočki","Priročnik za namestitev","","","","1","1","","1","1"]
["","Vrečka vijaka","","","","1","1","","1","1"]
["","Izpustni čep","","","","1","1","","1","1"]
["Hladilno sredstvo","Charge","","","TCO2Eq","2.5","2.5","","3.3","3.3"]
["","GWP","","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Polnjenje","","","kg","1.20","1.20","","1.60","1.60"]
["","Type","","","","R-410A","R-410A","","R-410A","R-410A"]
["Piping connections","Višinska razlika","IU - IU","Maks.","m","7.5","7.5","","7.5","7.5"]
["","","IU - OU","Maks.","m","15","15","","15","15"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 20m)","0,02 (za dolžino napeljave nad 20m)","","0,02 (za dolžino napeljave nad 20m)","0,02 (za dolžino napeljave nad 20m)"]
["","Skupna dolžina cevi","Sistem","Dejansko","m","30","30","","30","30"]
["Kompresor","Tip","","","","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor","","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor"]
["Mere","Enota","","Width","mm","765","765","","765","765"]
["","","","Depth","mm","285","285","","285","285"]
["","","","Višina","mm","550","550","","550","550"]
["Teža","Enota","","","kg","38","38","","42","42"]
["Power supply","Faza","","","","1~","1~","","1~","1~"]
["","Frekvenca","","","Hz","50","50","","50","50"]
["","Napetost","","","V","220-240","220-240","","220-240","220-240"]
["Opombe","","","","","(1) - Vsebuje fluorirane toplogredne pline","(1) - Vsebuje fluorirane toplogredne pline","","(1) - Vsebuje fluorirane toplogredne pline","(1) - Vsebuje fluorirane toplogredne pline"]
["Mere","Enota","","Višina","mm","","","550","","","550"]
["","","","Širina","mm","","","765","","","765"]
["","","","Globina","mm","","","285","","","285"]
["Teža","Enota","","","kg","","","38","","","42"]
["Kompresor","Tip","","","","","","Hermetično zaprt nihajni kompresor","","","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","°CDB","","","10","","","10"]
["","","","Maks.","°CDB","","","46","","","46"]
["","Gretje","Okolje","Min.","° CWB","","","-15","","","-15"]
["","","","Maks.","° CWB","","","15.5","","","15.5"]
["Raven zvočnega tlaka","Hlajenje","","Nom.","dBA","","","47","","","48"]
["","Gretje","","Nom.","dBA","","","48","","","50"]
["Hladilno sredstvo","Tip","","","","","","R-410A","","","R-410A"]
["","Polnitev","","","kg","","","1.20","","","1.60"]
["","Polnjenje","","","tCO2Eq","","","2.5","","","3.3"]
["","GWP","","","","","","2087.5","","","2087.5"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","","","20","","","20"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","","","0,02 (za dolžino napeljave nad 20m)","","","0,02 (za dolžino napeljave nad 20m)"]
["","Višinska razlika","IU - OU","Maks.","m","","","15","","","15"]
["","","IU - IU","Maks.","m","","","7.5","","","7.5"]
["","Skupna dolžina cevi","Sistem","Dejansko","m","","","30","","","30"]
["Standardni pripomočki","Installation manual","","","","","","1","","","1"]
["","Drain plug","","","","","","1","","","1"]
["","Screw bag","","","","","","1","","","1"]
["Napajanje","Faza","","","","","","1~","","","1~"]
["","Frekvenca","","","Hz","","","50","","","50"]
["","Napetost","","","V","","","220-240","","","220-240"]
["Standardni pripomočki","Sklop reduktorja","","","","","","","1","1"]
["","Reducer assembly","","","","","","","","","1"]