{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":68,"n_cols":7,"rows_kept":68,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXM-M"]
[]
[]
[]
[]
["","","","","","3AMXM52M3V1B","3AMXM52M2V1B"]
["Raven zvočnega tlaka","Gretje","","Nom.","dBA","47"]
["","Hlajenje","","Nom.","dBA","46"]
["Standardni pripomočki","Priročnik za namestitev","","","","1"]
["","Vrečka vijaka","","","","1"]
["","Izpustni čep","","","","1"]
["","Pokrovček izpusta (1)","","","","6"]
["","Pokrovček izpusta (2)","","","","3"]
["","Odlepite oznako za F-plin","","","","1"]
["","Oznaka dodatnega hladilnega sredstva","","","","1"]
["Hladilno sredstvo","Charge","","","TCO2Eq","1.2"]
["","GWP","","","","675"]
["","Charge","","","kg","1.8"]
["","Tip","","","","R-32"]
["Motor ventilatorja","Hitrost","Hlajenje","Izjwemno nizka","vrt/min","420"]
["","","Gretje","Izjwemno nizka","vrt/min","420"]
["Priključki napeljave","Višinska razlika","IU - IU","Maks.","m","7.5"]
["","","IU - OU","Maks.","m","15"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 30 m)"]
["","Skupna dolžina cevi","Sistem","Dejansko","m","50"]
["Kompresor","Tip","","","","Hermetično zaprt nihajni kompresor"]
["Mere","Enota","","Širina","mm","868"]
["","","","Globina","mm","320"]
["","","","Višina","mm","734"]
["Teža","Enota","","","kg","57"]
["Power supply","Phase","","","","1~"]
["","Frekvenca","","","Hz","50"]
["","Napetost","","","V","220-240"]
["Opombe","","","","","(1) - Vsebuje fluorirane toplogredne pline"]
["","","","","","(2) - Glejte ločeno risbo za obratovalno območje"]
["","","","","","(3) - Glejte ločeno risbo za električne podatke"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Izjemno nizka","m³/min","","24"]
["","","Ogrevanje","Izjemno nizka","m³/min","","24"]
["","","","Izjemno nizka","cfm","","847"]
["","","Ogrevanje","Izjemno nizka","cfm","","847"]
["Mere","Enota","","Višina","mm","","734"]
["","","","Širina","mm","","868"]
["","","","Globina","mm","","320"]
["Teža","Enota","","","kg","","57"]
["Motor ventilatorja","Hitrost","Hlajenje","Izjwemno nizka","vrt/min","","420"]
["","","Ogrevanje","Izjwemno nizka","vrt/min","","420"]
["Kompresor","Tip","","","","","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","°CDB","","-10"]
["","","","Maks.","°CDB","","46"]
["","Gretje","Okolje","Min.","° CWB","","-15"]
["","","","Maks.","° CWB","","18"]
["Raven zvočnega tlaka","Hlajenje","","Nom.","dBA","","46"]
["","Gretje","","Nom.","dBA","","47"]
["Hladilno sredstvo","Tip","","","","","R-32"]
["","Polnitev","","","kg","","1.80"]
["","Polnjenje","","","tCO2Eq","","1.2"]
["","GWP","","","","","675"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","","25"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","","0,02 (za dolžino napeljave nad 30 m)"]
["","Višinska razlika","IU - OU","Maks.","m","","15"]
["","","IU - IU","Maks.","m","","7.5"]
["","Skupna dolžina cevi","Sistem","Dejansko","m","","50"]
["Standardni pripomočki","Installation manual","","","","","1"]
["","Drain plug","","","","","1"]
["","Screw bag","","","","","1"]
["Napajanje","Faza","","","","","1~"]
["","Frekvenca","","","Hz","","50"]
["","Napetost","","","V","","220-240"]