{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-N7"]
[]
[]
[]
[]
["","","","","","3MXM40N2V1B7","3MXM52N2V1B7","3MXM68N2V1B7"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Izjemno nizka","m³/min","","","24.1"]
["","","Ogrevanje","Izjemno nizka","m³/min","","","24.1"]
["","","","Izjemno nizka","cfm","","","851"]
["","","Ogrevanje","Izjemno nizka","cfm","","","851"]
["Mere","Enota","","Višina","mm","734","734","734"]
["","","","Širina","mm","974","974","958"]
["","","","Globina","mm","401","401","340"]
["Teža","Enota","","","kg","57","57","62"]
["Motor ventilatorja","Hitrost","Hlajenje","Izjwemno nizka","vrt/min","420","420"]
["","","Ogrevanje","Izjwemno nizka","vrt/min","420","420"]
["Kompresor","Tip","","","","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","°CDB","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46"]
["","Gretje","Okolje","Min.","° CWB","","","-15"]
["","","","Maks.","° CWB","","","24"]
["Raven zvočnega tlaka","Hlajenje","","Nom.","dBA","46","46","48"]
["","Gretje","","Nom.","dBA","47","47","48"]
["Hladilno sredstvo","Tip","","","","R-32","R-32","R-32"]
["","Polnitev","","","kg","1.8","1.8","2"]
["","Polnjenje","","","tCO2Eq","1.22","1.22"]
["","GWP","","","","675","675","675"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","25","25 (1)","25"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 30 m)","0,02 (za dolžino napeljave nad 30 m)","0,02 (za dolžino napeljave nad 30 m)"]
["","Višinska razlika","IU - OU","Maks.","m","15.0","15.0","15"]
["","","IU - IU","Maks.","m","7.5","7.5","7.5"]
["","Skupna dolžina cevi","Sistem","Dejansko","m","50","50 (2)","50"]
["Standardni pripomočki","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Napajanje","Faza","","","","1~","1~","1~"]
["","Frekvenca","","","Hz","50","50","50"]
["","Napetost","","","V","220-240","220-240","220-440"]
["Opombe","","","","","(1) - Za en prostor","(1) - Za en prostor"]
["","","","","","(2) - Za kombinacijo s CVXM-A, FVXM-A - največja dolžina cevne napeljave je 30 m.","(2) - Za kombinacijo s CVXM-A, FVXM-A - največja dolžina cevne napeljave je 30 m."]
["Kompresor","Tip","","","","","","Hermetično zaprt nihajni kompresor"]
["Standardni pripomočki","Priročnik za namestitev","","","","","","1"]
["","Pokrovček izpusta","","","","","","3"]
["","Izpustni čep","","","","","","1"]
["","Sklop reduktorja","","","","","","1"]
["","Vrečka vijaka","","","","","","1"]
["Razpon energetske učinkovitosti","","","","","","","A+++ ~ D"]