{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":8,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXS-E"]
[]
[]
[]
[]
["","","","","","4MXS80E3V3B2","4MXS80E3V3B","4MXS80E7V3B"]
["Mere","Enota","","Višina","mm","770","770"]
["","","","Širina","mm","900","900"]
["","","","Globina","mm","320","320"]
["Teža","Enota","","","kg","72","72"]
["Kompresor","Tip","","","","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["","Ogrevanje","Okolje","Min.","° CWB","-15","-15"]
["","","","Maks.","° CWB","18","18"]
["Raven zvočnega tlaka","Hlajenje","","Nom.","dBA","48","48"]
["","Gretje","","Nom.","dBA","49","49"]
["Hladilno sredstvo","Tip","","","","R-410A","R-410A"]
["","Charge","","","kg","2.99","2.99"]
["","GWP","","","","2,087.5","2,087.5"]
["Priključki cevne napeljave","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 30 m)","0,02 (za dolžino napeljave nad 30 m)"]
["","Višinska razlika","IU - OU","Maks.","m","15","15"]
["","","IU - IU","Maks.","m","7.5","7.5"]
["","Skupna dolžina cevi","Sistem","Dejansko","m","70","70"]
["Standardni pripomočki","Priročnik za namestitev","","","","1","1"]
["","Izpustni čep","","","","1","1"]
["","Sklop reduktorja","","","","1","1"]
["Power supply","Faza","","","","1~","1~"]
["","Frekvenca","","","Hz","50","50"]
["","Napetost","","","V","230","230"]
["Opombe","","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5 m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5 m"]
["","","","","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5 m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5 m"]
["","","","","","(3) - Vsebuje fluorirane toplogredne pline","(3) - Vsebuje fluorirane toplogredne pline"]
["Mere","Enota","","Višina","mm","","","770"]
["","","","Širina","mm","","","900"]
["","","","Globina","mm","","","320"]
["Teža","Enota","","","kg","","","72"]
["Kompresor","Tip","","","","","","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","°CDB","","","-10"]
["","","","Maks.","°CDB","","","46"]
["","Gretje","Okolje","Min.","° CWB","","","-15"]
["","","","Maks.","° CWB","","","15.5"]
["Raven zvočnega tlaka","Hlajenje","","Nom.","dBA","","","48"]
["","Gretje","","Nom.","dBA","","","49"]
["Hladilno sredstvo","Tip","","","","","","R-410A"]
["","Polnitev","","","kg","","","2.99"]
["","Polnjenje","","","tCO2Eq","","","6.2"]
["","GWP","","","","","","2087.5"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","","","25"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","","","0,02 (za dolžino napeljave nad 30 m)"]
["","Višinska razlika","IU - OU","Maks.","m","","","15"]
["","","IU - IU","Maks.","m","","","7.5"]
["","Skupna dolžina cevi","Sistem","Dejansko","m","","","70"]
["Standardni pripomočki","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["Napajanje","Faza","","","","","","1~"]
["","Frekvenca","","","Hz","","","50"]
["","Napetost","","","V","","","230"]