{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MWXM-A9"]
[]
[]
[]
[]
["","","","","","5MWXM68A2V1B9","5MWXM90A2V1B9"]
["Mere","Enota","","Višina","mm","734","734"]
["","","","Širina","mm","1040","1040"]
["","","","Globina","mm","408","408"]
["Teža","Enota","","","kg","69","73"]
["Kompresor","Tip","","","","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["Raven zvočnega tlaka","Hlajenje","","Nom.","dBA","48","52"]
["","Gretje","","Nom.","dBA","49","53"]
["Hladilno sredstvo","Tip","","","","R-32","R-32"]
["","Polnitev","","","kg","2","2.4"]
["","Polnjenje","","","tCO2Eq","1.35","1.62"]
["","GWP","","","","675","675"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","25 (2)","25 (3)"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 30 m)","0,02 (za dolžino napeljave nad 30 m)"]
["","Višinska razlika","IU - OU","Maks.","m","15 (3)","15"]
["","","IU - IU","Maks.","m","7.5 (3)","7.5 (3)"]
["","Skupna dolžina cevi","Sistem","Dejansko","m","60","75"]
["Standardni pripomočki","Priročnik za namestitev","","","","1","1"]
["","Pokrovček izpusta","","","","3","3"]
["","Izpustni čep","","","","1","1"]
["","Sklop reduktorja","","","","1","1"]
["","Vrečka vijaka","","","","2","2"]
["Razpon energetske učinkovitosti","","","","","A+++ ~ D","A+++ ~ D"]
["Napajanje","Faza","","","","1~","1~"]
["","Frekvenca","","","Hz","50","50"]
["","Napetost","","","V","220-440","220-240"]
["Opombe","","","","","(1) - Glejte ločeno risbo za obratovalno območje","(1) - Glejte ločeno risbo za obratovalno območje"]
["","","","","","(2) - Za en prostor","(2) - Za en prostor"]
["","","","","","(3) - Za en prostor (za kombinacijo s FBA71/100/125 in EKHWET ter CKHWS glejte navodila za vgradnjo)","(3) - Za en prostor (za kombinacijo s FBA71/100/125 in EKHWET ter CKHWS glejte navodila za vgradnjo)"]
["","","","","","(4) - Vsebuje fluorirane toplogredne pline","(4) - Vsebuje fluorirane toplogredne pline"]