{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MXM-M"]
[]
[]
[]
[]
["","","","","","5MXM90M2V1B"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Izjemno nizka","m³/min","24.1"]
["","","Ogrevanje","Izjemno nizka","m³/min","24.1"]
["","","","Izjemno nizka","cfm","851"]
["","","Ogrevanje","Izjemno nizka","cfm","851"]
["Mere","Enota","","Višina","mm","734"]
["","","","Širina","mm","320"]
["","","","Globina","mm","868"]
["Teža","Enota","","","kg","68"]
["Kompresor","Tip","","","","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","°CDB","-10"]
["","","","Maks.","°CDB","46"]
["","Gretje","Okolje","Min.","° CWB","-15"]
["","","","Maks.","° CWB","18"]
["Raven zvočnega tlaka","Hlajenje","","Nom.","dBA","52"]
["","Gretje","","Nom.","dBA","52"]
["Hladilno sredstvo","Tip","","","","R-32"]
["","Polnitev","","","kg","2.4"]
["","Polnjenje","","","tCO2Eq","1.6"]
["","GWP","","","","675"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","25"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 30 m)"]
["","Višinska razlika","IU - OU","Maks.","m","15"]
["","","IU - IU","Maks.","m","7.5"]
["","Skupna dolžina cevi","Sistem","Dejansko","m","75"]
["Standardni pripomočki","Installation manual","","","","1"]
["","Drain cap","","","","9"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Screw bag","","","","1"]
["Napajanje","Faza","","","","1~"]
["","Frekvenca","","","Hz","50"]
["","Napetost","","","V","220-240"]