{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":8,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C / AZQS-B(8)V1"]
[]
[]
[]
[]
["","","","","ABQ71CV1 / AZQS71B2V1B","ABQ100CV1 / AZQS100B8V1B","ABQ125CV1 / AZQS125B8V1B","ABQ140CV1 / AZQS140B8V1B"]
["Hladilna kapaciteta","Nom.","","kW","6.8","9.5","12.1","13.0 (1)"]
["Hlajenje prostora","SEER","","","4.65","4.65","","5.01"]
["","Letna poraba energije","","kWh/a","512","716","","1,559"]
["","Zmogljivost","Pdizajn","kW","6.80","9.50","","13.0"]
["","Razred energijske učinkovitosti","","","B","B"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","5.65","6.78","","12.3"]
["","SCOP/A","","","3.80","3.80","","3.58"]
["","Razred energijske učinkovitosti","","","A","A"]
["","Letna poraba energije","","kWh/a","2,082","2,498","","4,811"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","1,165","1,813","2,153"]
["","EER","","","2.91","2.62","2.81","3.36 (3)"]
["","COP","","","3.51","3.42","3.41"]
["","Direktiva o energijskih oznakah","Hlajenje","","C","D","C"]
["","","Ogrevanje","","B","B","B"]
["Grelna kapaciteta","Nom.","","kW","7.5","10.8","13.5","15.5 (2)"]
["Opombe","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m"]
["","","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m"]
["","","","","","(3) - PED: sestava = kategorija l : izključena iz obsega PED zaradi člena 1, točke 3.6 v okviru 97/23/EC","(3) - PED: sestava = kategorija l : izključena iz obsega PED zaradi člena 1, točke 3.6 v okviru 97/23/EC","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["","","","","","(4) - Minimalna vrednost Ssc (kratkostične moči): Oprema je skladna z EN 61000-3-2","(4) - Minimalna vrednost Ssc (kratkostične moči): Oprema je skladna z EN 61000-3-2"]
["","","","","","(5) - Glejte ločeno risbo za električne podatke","(5) - Glejte ločeno risbo za električne podatke"]
["","","","","","(6) - Vsebuje fluorirane toplogredne pline","(6) - Vsebuje fluorirane toplogredne pline"]