{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C / AZQS-BY1"]
[]
[]
[]
[]
["","","","","ABQ100CV1 / AZQS100B7Y1B","ABQ125CV1 / AZQS125B7Y1B"]
["Hladilna kapaciteta","Nom.","","kW","9.5","12.1 (1)"]
["Hlajenje prostora","SEER","","","4.65","4.68"]
["","Letna poraba energije","","kWh/a","716","1,550"]
["","Zmogljivost","Pdizajn","kW","9.50","12.1"]
["","Razred energijske učinkovitosti","","","B"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","6.78","8.13"]
["","SCOP/A","","","3.80","3.41"]
["","Razred energijske učinkovitosti","","","A"]
["","Letna poraba energije","","kWh/a","2,498","3,340"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","1,813"]
["","EER","","","2.62","2.27 (3)"]
["","COP","","","3.42"]
["","Direktiva o energijskih oznakah","Hlajenje","","D"]
["","","Ogrevanje","","B"]
["Grelna kapaciteta","Nom.","","kW","10.8","13.5 (2)"]
["Opombe","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m"]
["","","","","(2) - Letna poraba energije je v skladu z direktivo 2002/31/EC za označevanje energije","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m"]
["","","","","(3) - SEER in SCOP sta v skladu z EN 14825","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["","","","","(4) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]