{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":9,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C"]
[]
[]
[]
[]
["","","","","","ABQ71CV1","ABQ100CV1","ABQ125CV1","ABQ140CV1"]
["Standardni pripomočki","Priročnik za namestitev","","","","Priročnik za namestitev"]
["","Priročnik za upravljanje","","","","Priročnik za upravljanje"]
["","Vijak+Podložka","","","","Vijak+Podložka"]
["","Brezžičen daljinski upravljalnik","","","","Brezžičen daljinski upravljalnik"]
["","Pokrivna zaporna mreža","","","","Pokrivna zaporna mreža"]
["","Baterija","","","","Baterija"]
["Cevni priklj.","Tekočina","","Zun. premer","mm","9.52"]
["","Plin","","OD","mm","15.88"]
["","Drain","","","","19.05"]
["Power input","Hlajenje","","Nom.","kW","0.128"]
["","Gretje","","Nom.","kW","0.128"]
["Raven zvočne moči","Hlajenje","","","dBA","64"]
["","Gretje","","","dBA","64"]
["Mere","Enota","","Width","mm","600"]
["","","","Globina","mm","1,007"]
["","","","Height","mm","285"]
["Casing","Material","","","","Galvanizirano jeklo"]
["Teža","Unit","","","kg","35"]
["Ventilator","Zunanji statični tlak","","Visok","Pa","90"]
["","","","Nom.","Pa","77"]
["","","","Nizko","Pa","64"]
["Power supply","Phase","","","","1~"]
["","Frekvenca","","","Hz","50"]
["","Ime","","","","V1"]
["","Napetost","","","V","220-240"]
["Vhodna moč","Gretje","","Nom.","kW","","0.109"]
["","Hlajenje","","Nom.","kW","","0.109"]
["Ventilator","Zunanji statični tlak","","Visok","Pa","","70","150","150"]
["","","","Nizek","Pa","","45","111","92"]
["Ohišje","Material","","","","","Galvanizirano jeklo"]
["Mere","Enota","","Višina","mm","","378","378","378"]
["","","","Širina","mm","","541","1300","1500"]
["","","","Globina","mm","","1045","541","541"]
["Teža","Enota","","","kg","","44","50","56"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","","22.7","40.5","48.7"]
["","","","Nom.","m³/min","","20.5","37","44"]
["","","","Nizko","m³/min","","18.3","34.8","37.9"]
["","","Gretje","Visok","m³/min","","22.7","40.5","48.7"]
["","","","Nom.","m³/min","","20.5","37.4","43.9"]
["","","","Nizko","m³/min","","18.3","34.8","37.9"]
["","Zunanji statični tlak","","Nom.","Pa","","57","128","122"]
["Raven zvočne moči","Hlajenje","","","dBA","","60","72","73"]
["","Gretje","","","dBA","","60","72","73"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","","41","53","55"]
["","","","Nom.","dBA","","38"]
["","","","Nizko","dBA","","36","50","50"]
["","Gretje","","Visok","dBA","","41","53","55"]
["","","","Nom.","dBA","","38"]
["","","","Nizko","dBA","","36","50","50"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","","9.52","9.52","9.52"]
["","Plin","","Zun. premer","mm","","15.88","15.9","15.9"]
["","Izpust","","","","","19.05"]
["Standardni pripomočki","Installation manual","","","","","Installation manual"]
["","Wireless remote control","","","","","Wireless remote control"]
["","Cover lock grill","","","","","Cover lock grill"]
["","Battery","","","","","Battery"]
["","Screw+Washer","","","","","Screw+Washer"]
["","Operation manual","","","","","Operation manual"]
["Napajanje","Faza","","","","","1~"]
["","Frekvenca","","","Hz","","50"]
["","Napetost","","","V","","220-240"]
["Hladilna kapaciteta","Skupna kapaciteta","","Nom.","kW","","","12.10","13.00"]
["Zmogljivost gretja","Skupna kapaciteta","","Nom.","kW","","","13.5","15.5"]
["Ohišje","Barva","","","","","","Pocinkana pločevina / nepobarvana","Pocinkana pločevina / nepobarvana"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Srednja","m³/min","","","37","44"]
["","","Ogrevanje","Srednja","m³/min","","","37.4","43.9"]
["Raven zvočnega tlaka","Hlajenje","","Srednja","dBA","","","52","53"]
["","Ogrevanje","","Srednja","dBA","","","52","53"]
["Krmilni sistemi","Infrardeči daljinski upravljalnik","","","","","","ARCWLA","ARCWLA"]