{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A / ARXM-A"]
[]
[]
[]
[]
["","","","","ADEA50A2VEB / ARXM50A5V1B","ADEA60A2VEB / ARXM60A5V1B","ADEA71A2VEB / ARXM71A5V1B"]
["Hladilna kapaciteta","Nom.","","kW","5.00","5.7","6.8"]
["","Maks.","","kW","","","6.98"]
["Grelna kapaciteta","Nom.","","kW","5.50","7","7.5"]
["","Maks.","","kW","","","7.66"]
["Nom. učink.","EER","","","3.27","3.43","2.95"]
["","COP","","","3.74","3.63","3.49"]
["","Letna por.energ.","","kWh","765","831","1153"]
["Imenska učinkovitost","Direktiva o energijskih oznakah","Hlajenje","","A","A","C"]
["Nazivna učinkovitost","Direktiva o energijskih oznakah","Ogrevanje","","A","A","B"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","A+","A+","A"]
["","Zmogljivost","Pdizajn","kW","5.00","5.7","6.8"]
["","SEER","","","5.65","5.74","5.35"]
["","Letna poraba energije","","kWh/a","310","347","445"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","A+","A+","A"]
["","Zmogljivost","Pdizajn","kW","4.40","4.6","6"]
["","SCOP/A","","","4.00","4","3.8"]
["","Pdh Zmogljvost ogrevanja pri -10°","","kW","3.73","4","4.83"]
["","Letna poraba energije","","kWh/a","1538","1610","2209"]
["Opombe","","","","","(1) - Glejte ločeno risbo za obratovalno območje","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m"]
["","","","","","(2) - Glejte ločeno risbo za električne podatke","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]
["","","","","","(3) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(3) - Glejte ločeno risbo za obratovalno območje"]
["","","","","","(4) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(4) - Glejte ločeno risbo za električne podatke"]