{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A / ARXM-A9"]
[]
[]
[]
[]
["","","","","ADEA35A2VEB / ARXM35A5V1B9","ADEA50A2VEB / ARXM50A5V1B9"]
["Hladilna kapaciteta","Nom.","","kW","3.4","5"]
["Grelna kapaciteta","Nom.","","kW","4","5.5"]
["Nom. učink.","EER","","","3.76","3.27"]
["","COP","","","3.97","3.74"]
["","Letna por.energ.","","kWh","452","765"]
["Imenska učinkovitost","Direktiva o energijskih oznakah","Hlajenje","","A","A"]
["Nazivna učinkovitost","Direktiva o energijskih oznakah","Ogrevanje","","A","A"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","A+","A+"]
["","Zmogljivost","Pdizajn","kW","3.4","5"]
["","SEER","","","5.9","5.65"]
["","Letna poraba energije","","kWh/a","202","310"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","A+","A+"]
["","Zmogljivost","Pdizajn","kW","2.9","4.4"]
["","SCOP/A","","","4.07","4"]
["","Pdh Zmogljvost ogrevanja pri -10°","","kW","2.32","3.73"]
["","Letna poraba energije","","kWh/a","997","1538"]
["Razpon energetske učinkovitosti","","","","A+++ ~ D","A+++ ~ D"]
["Opombe","","","","(1) - Glejte ločeno risbo za obratovalno območje","(1) - Glejte ločeno risbo za obratovalno območje"]
["","","","","(2) - Glejte ločeno risbo za električne podatke","(2) - Glejte ločeno risbo za električne podatke"]
["","","","","(3) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(3) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m"]
["","","","","(4) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(4) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]