{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A / ARXM-N9"]
[]
[]
[]
[]
["","","","","ADEA71A2VEB / ARXM71N2V1B9"]
["Hladilna kapaciteta","Nom.","","kW","6.80"]
["","Maks.","","kW","6.98"]
["Grelna kapaciteta","Nom.","","kW","7.50"]
["","Maks.","","kW","7.66"]
["Nom. učink.","EER","","","2.95"]
["","COP","","","3.49"]
["","Letna por.energ.","","kWh","1153"]
["Imenska učinkovitost","Direktiva o energijskih oznakah","Hlajenje","","C"]
["Nazivna učinkovitost","Direktiva o energijskih oznakah","Ogrevanje","","B"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","A"]
["","Zmogljivost","Pdizajn","kW","6.80"]
["","SEER","","","5.35"]
["","Letna poraba energije","","kWh/a","445"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","A"]
["","Zmogljivost","Pdizajn","kW","6.00"]
["","SCOP/A","","","3.80"]
["","Pdh Zmogljvost ogrevanja pri -10°","","kW","4.83"]
["","Letna poraba energije","","kWh/a","2209"]
["Razpon energetske učinkovitosti","","","","A+++ ~ D"]
["Opombe","","","","(1) - Glejte ločeno risbo za obratovalno območje"]
["","","","","(2) - Glejte ločeno risbo za električne podatke"]
["","","","","(3) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m"]
["","","","","(4) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]