{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":6,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A / AZQS-B(8)V1"]
[]
[]
[]
[]
["","","","","ADEA100A2VEB / AZQS100B8V1B","ADEA125A2VEB / AZQS125B8V1B"]
["Hladilna kapaciteta","Nom.","","kW","9.50","12.10"]
["Hlajenje prostora","SEER","","","5.10","4.83"]
["","Letna poraba energije","","kWh/a","652","1,504"]
["","Zmogljivost","Pdizajn","kW","9.50","12.10"]
["","Razred energijske učinkovitosti","","","A"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","7.60","7.93"]
["","SCOP/A","","","3.81","3.50"]
["","Razred energijske učinkovitosti","","","A"]
["","Letna poraba energije","","kWh/a","2,793","3,167"]
["Nazivna učinkovitost","EER","","","","2.27"]
["Grelna kapaciteta","Nom.","","kW","10.80","13.50"]
["Opombe","","","","(1) - Glejte ločeno risbo za obratovalno območje","(1) - Glejte ločeno risbo za obratovalno območje"]
["","","","","(2) - Glejte ločeno risbo za električne podatke","(2) - Glejte ločeno risbo za električne podatke"]
["","","","","(3) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(3) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m"]
["","","","","(4) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","(4) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m"]