{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AHQ-C / AZQS-BY1 UK"]
[]
[]
[]
[]
["","","","","AHQ100CV1 / AZQS100B7Y1B UK","AHQ125CV1 / AZQS125B7Y1B UK","AHQ140CV1 / AZQS140B7Y1B UK"]
["Hladilna kapaciteta","Nom.","","kW","9.5","12.1","13.0"]
["Hlajenje prostora","SEER","","","4.60"]
["","Letna poraba energije","","kWh/a","716"]
["","Zmogljivost","Pdizajn","kW","9.50"]
["","Razred energijske učinkovitosti","","","B"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","7.60"]
["","SCOP/A","","","3.80"]
["","Razred energijske učinkovitosti","","","A"]
["","Letna poraba energije","","kWh/a","2,800"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","1,810","2,300"]
["","EER","","","2.62","2.63","3.01"]
["","COP","","","3.41","3.61","3.41"]
["","Direktiva o energijskih oznakah","Hlajenje","","D","D"]
["","","Ogrevanje","","B","A"]
["Zmogljivost gretja","Nom.","","kW","10.8","13.5","15.5"]
["Opombe","","","","(1) - Letna poraba energije je v skladu z direktivo 2002/31/EC za označevanje energije","(1) - Letna poraba energije je v skladu z direktivo 2002/31/EC za označevanje energije","(1) - Letna poraba energije je v skladu z direktivo 2002/31/EC za označevanje energije"]
["","","","","(2) - SEER in SCOP sta v skladu z EN 14825","(2) - SEER in SCOP sta v skladu z EN 14825","(2) - SEER in SCOP sta v skladu z EN 14825"]
["","","","","(3) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(3) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(3) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]