{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":9,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AHQ-C"]
[]
[]
[]
[]
["","","","","","AHQ71CV1","AHQ100CV1","AHQ125CV1","AHQ140CV1"]
["Vhodna moč","Gretje","","Nom.","kW","0.106","0.149"]
["","Hlajenje","","Nom.","kW","0.106","0.149"]
["Ventilator","Zunanji statični tlak","","Visok","Pa","0","0","0","0"]
["","","","Nizek","Pa","0","0","0","0"]
["Hladilna kapaciteta","Skupna kapaciteta","","Nom.","kW","","","12.10","13.00"]
["Zmogljivost gretja","Skupna kapaciteta","","Nom.","kW","","","13.5","15.5"]
["Ohišje","Barva","","","","Bela","Bela","Bela","Bela"]
["","Material","","","","Galvanizirano jeklo","Galvanizirano jeklo"]
["Mere","Enota","","Višina","mm","260","260","260","285"]
["","","","Širina","mm","1320","1538","1790","1900"]
["","","","Globina","mm","634","634","634","680"]
["Teža","Enota","","","kg","38","45","65","70"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","23.8","31.1","34.4","43.9"]
["","","","Nom.","m³/min","21.3","27.8","31","39"]
["","","","Srednja","m³/min","","","31","39"]
["","","","Nizko","m³/min","18.9","24.8","27.2","28.3"]
["","","Gretje","Visok","m³/min","23.8","31.1","34.4","43.9"]
["","","","Nom.","m³/min","21.3","27.8","30.6","39.1"]
["","","Ogrevanje","Srednja","m³/min","","","30.6","39.1"]
["","","Gretje","Nizko","m³/min","18.9","24.8","27.2","28.3"]
["","Zunanji statični tlak","","Nom.","Pa","0","0","0","0"]
["Raven zvočne moči","Hlajenje","","","dBA","59","64","65","71"]
["","Gretje","","","dBA","62","64","65","71"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","49","52","52","56"]
["","","","Nom.","dBA","48","47"]
["","","","Srednja","dBA","","","50","53"]
["","","","Nizko","dBA","46","46","49","46"]
["","Gretje","","Visok","dBA","49","52","52","56"]
["","Ogrevanje","","Srednja","dBA","","","50","53"]
["","Gretje","","Nom.","dBA","48","47"]
["","","","Nizko","dBA","46","46","49","46"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","9.52","9.52","9.52","9.52"]
["","Plin","","Zun. premer","mm","15.88","15.88","15.9","15.9"]
["","Izpust","","","","19.05","19.05"]
["Krmilni sistemi","Infrardeči daljinski upravljalnik","","","","ARCWLA","ARCWLA","ARCWLA","ARCWLA"]
["","Ožičeni daljinski krmilnik","","","","ARCWB","ARCWB"]
["Standardni pripomočki","Installation manual","","","","Installation manual","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","Wireless remote control"]
["","Battery","","","","Battery","Battery"]
["","Odtočna cev","","","","Drain pipe","Drain pipe"]
["","Screw for wireless remote","","","","Screw for wireless remote","Screw for wireless remote"]
["","Ferrite Core","","","","Ferrite Core","Ferrite Core"]
["","Installation manual (Ferrite Core)","","","","Installation manual (Ferrite Core)","Installation manual (Ferrite Core)"]
["","Outdoor wiring diagram","","","","Outdoor wiring diagram","Outdoor wiring diagram"]
["","Operation manual","","","","Operation manual","Operation manual"]
["","Drain hose","","","","Drain hose","Drain hose"]
["Napajanje","Faza","","","","1~","1~"]
["","Frekvenca","","","Hz","50","50"]
["","Napetost","","","V","220-240","220-240"]