{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":10,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-A"]
[]
[]
[]
[]
["","","","","","ARXM25A5V1B","ARXM35A5V1B","ARXM50A5V1B","ARXM60A5V1B","ARXM71A5V1B"]
["Mere","Enota","","Višina","mm","610","610","734","734","734"]
["","","","Širina","mm","923","923","954","954","954"]
["","","","Globina","mm","367","367","401","401","401"]
["Teža","Enota","","","kg","36","36","49","49","49"]
["Motor ventilatorja","Hitrost","Hlajenje","Izjwemno nizka","vrt/min","600","600","500"]
["Kompresor","Tip","","","","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","°CDB","-10","-10","-10","-10","-10"]
["","","","Maks.","°CDB","50","50","50 (1), 46 (1)","46","46"]
["","Gretje","Okolje","Min.","° CWB","-21","-21","-21 (1), -15 (1)","-15","-15"]
["","","","Maks.","° CWB","18","18","18","18","18"]
["Raven zvočnega tlaka","Hlajenje","","Nom.","dBA","46","47","48","48","52"]
["","Gretje","","Nom.","dBA","47","49","49","49","52"]
["Hladilno sredstvo","Tip","","","","R-32","R-32","R-32","R-32","R-32"]
["","Polnitev","","","kg","0.95","0.95","1.1","1.15","1.15"]
["","Polnjenje","","","tCO2Eq","0.65","0.65","0.75","0.78","0.78"]
["","GWP","","","","675","675","675","675","675"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","20","20","30","30","30"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)","0035 (za cevno napeljavo daljšo od 10 m)"]
["","Višinska razlika","IU - OU","Maks.","m","15","15","20","20","20"]
["Standardni pripomočki","Priročnik za namestitev","","","","1","1","1","1","1"]
["","Izpustni spoj","","","","1","1","1"]
["","Oznaka polnitve hladilnega sredstva","","","","1","1","1","1","1"]
["","Večjezikovne oznake za fluorirane toplogredne pline","","","","1","1","1","1","1"]
["","Splošni varnostni previdnostni ukrepi","","","","1","1","1"]
["","Energetska oznaka LOT10","","","","1","1","1"]
["","Pokrovček izpusta","","","","3","3","1","3","3"]
["Razpon energetske učinkovitosti","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Napajanje","Faza","","","","1~","1~","1~","1~","1~"]
["","Frekvenca","","","Hz","50","50","50","50","50"]
["","Napetost","","","V","220-240","220-240","220-240","220-240","220-240"]
["Opombe","","","","","(1) - Glejte ločeno risbo za obratovalno območje","(1) - Glejte ločeno risbo za obratovalno območje","(1) - Glejte ločeno risbo za obratovalno območje","(1) - Glejte ločeno risbo za obratovalno območje","(1) - Glejte ločeno risbo za obratovalno območje"]
["","","","","","(2) - Glejte ločeno risbo za električne podatke","(2) - Glejte ločeno risbo za električne podatke","(2) - Glejte ločeno risbo za električne podatke","(2) - Glejte ločeno risbo za električne podatke","(2) - Glejte ločeno risbo za električne podatke"]
["","","","","","(3) - Vsebuje fluorirane toplogredne pline","(3) - Vsebuje fluorirane toplogredne pline","(3) - Vsebuje fluorirane toplogredne pline","(3) - Vsebuje fluorirane toplogredne pline","(3) - Vsebuje fluorirane toplogredne pline"]
["Standardni pripomočki","ARXM50A5V1B","","","","","","1"]
["","Izpustni čep","","","","","","","1","1"]