{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-A8"]
[]
[]
[]
[]
["","","","","","ARXM50A5V1B8"]
["Mere","Enota","","Višina","mm","610"]
["","","","Širina","mm","923"]
["","","","Globina","mm","367"]
["Teža","Enota","","","kg","40"]
["Motor ventilatorja","Hitrost","Hlajenje","Izjwemno nizka","vrt/min","600"]
["Kompresor","Tip","","","","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","°CDB","-10"]
["","","","Maks.","°CDB","50 (1), 46 (1)"]
["","Gretje","Okolje","Min.","° CWB","-21 (1), -15 (1)"]
["","","","Maks.","° CWB","18"]
["Raven zvočnega tlaka","Hlajenje","","Nom.","dBA","48"]
["","Gretje","","Nom.","dBA","49"]
["Hladilno sredstvo","Tip","","","","R-32"]
["","Polnitev","","","kg","0.95"]
["","Polnjenje","","","tCO2Eq","0.65"]
["","GWP","","","","675"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","30"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 10m)"]
["","Višinska razlika","IU - OU","Maks.","m","20"]
["Standardni pripomočki","Installation manual","","","","1"]
["","Drain joint","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","LOT10 Energy Label","","","","1"]
["","Drain cap","","","","3"]
["Napajanje","Faza","","","","1~"]
["","Frekvenca","","","Hz","50"]
["","Napetost","","","V","220-240"]
["Opombe","","","","","(1) - Glejte ločeno risbo za obratovalno območje"]
["","","","","","(2) - Glejte ločeno risbo za električne podatke"]
["","","","","","(3) - Vsebuje fluorirane toplogredne pline"]