{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":8,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-M9"]
[]
[]
[]
[]
["","","","","","ARXM25M3V1B9","ARXM35M3V1B9","ARXM50M3V1B9"]
["Mere","Enota","","Višina","mm","550","550","735"]
["","","","Širina","mm","765","765","825"]
["","","","Globina","mm","285","285","300"]
["Teža","Enota","","","kg","32","32","47"]
["Kompresor","Tip","","","","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","° CDB","-10","-10","-10"]
["","","","Maks.","° CDB","46","46","46"]
["","Gretje","Okolje","Min.","° CWB","10","10","10"]
["","","","Maks.","° CWB","18","18","18"]
["Raven zvočnega tlaka","Hlajenje","","Nom.","dBA","46","49","48"]
["","Gretje","","Nom.","dBA","47","49","49"]
["Hladilno sredstvo","Tip","","","","R-32","R-32","R-32"]
["","Polnitev","","","kg","0.76","0.76","1.40"]
["","Polnjenje","","","tCO2Eq","0.52","0.52","0.95"]
["","GWP","","","","675.0","675.0","675"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","20.0","20.0","30"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)"]
["","Višinska razlika","IU - OU","Maks.","m","20.0","20.0","20"]
["Standardni pripomočki","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["Napajanje","Faza","","","","1~","1~","1~"]
["","Frekvenca","","","Hz","50","50","50"]
["","Napetost","","","V","220-240","220-240","220-240"]
["Opombe","","","","","(1) - Vsebuje fluorirane toplogredne pline","(1) - Vsebuje fluorirane toplogredne pline","(1) - Glejte ločeno risbo za obratovalno območje"]