{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R9"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B9","ARXM35R5V1B9"]
["Raven zvočnega tlaka","Gretje","","Nom.","dBA","","49.0"]
["","Hlajenje","","Nom.","dBA","","49.0"]
["Standardni pripomočki","Izpustni čep","","","","","1"]
["","Priročnik za namestitev","","","","","1"]
["","Oznaka polnitve hladilnega sredstva","","","","","1"]
["","Večjezikovne oznake za fluorirane toplogredne pline","","","","","1"]
["","Splošni varnostni previdnostni ukrepi","","","","","1"]
["Hladilno sredstvo","Charge","","","TCO2Eq","","0.52"]
["","GWP","","","","","675"]
["","Polnitev","","","kg","","0.76"]
["","Tip","","","","","R-32"]
["Delovni doseg","Hlajenje","Okolje","Maks.","°CDB","","50 (4), 46 (5)"]
["","","","Min.","°CDB","","-10"]
["Piping connections","Višinska razlika","IU - OU","Maks.","m","","15"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","","0,02 (za dolžino napeljave nad 10m)"]
["Kompresor","Type","","","","","Hermetično zaprt nihajni kompresor"]
["Mere","Enota","","Širina","mm","","840"]
["","","","Globina","mm","","350"]
["","","","Višina","mm","","552"]
["Teža","Enota","","","kg","","32"]
["Power supply","Phase","","","","","1~"]
["","Frekvenca","","","Hz","","50"]
["","Napetost","","","V","","220-240"]
["Opombe","","","","","(1) - Mogoče samo v kombinaciji z ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Vsebuje fluorirane toplogredne pline"]
["","","","","","(2) - Mogoče samo v kombinaciji z ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Glejte ločeno risbo za obratovalno območje"]
["","","","","","","(3) - Glejte ločeno risbo za električne podatke"]
["","","","","","","(4) - Mogoče samo v kombinaciji z ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B"]
["","","","","","","(5) - Mogoče samo v kombinaciji z ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B"]
["Mere","Enota","","Višina","mm","552"]
["","","","Širina","mm","840"]
["","","","Globina","mm","350"]
["Teža","Enota","","","kg","32"]
["Kompresor","Tip","","","","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","°CDB","-10"]
["","","","Maks.","°CDB","50 (4), 46 (5)"]
["Raven zvočnega tlaka","Hlajenje","","Nom.","dBA","46.0"]
["","Gretje","","Nom.","dBA","47.0"]
["Hladilno sredstvo","Polnitev","","","kg","0.76"]
["","Polnjenje","","","tCO2Eq","0.52"]
["","GWP","","","","675"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","20"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 10m)"]
["","Višinska razlika","IU - OU","Maks.","m","15"]
["Standardni pripomočki","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Napajanje","Frekvenca","","","Hz","50"]