{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":10,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L"]
[]
[]
[]
[]
["","","","","","ARXS50L2V1B","ARXS71L2V1B","ARXS25L2V1B (Archived)","ARXS35L2V1B (Archived)","ARXS60L2V1B (Archived)"]
["Raven zvočnega tlaka","Gretje","","Visok","dBA","","","47","48"]
["","","","Nom.","dBA","","52","","","49"]
["","Hlajenje","","Visok","dBA","","","46","48"]
["","","","Nom.","dBA","","52","","","49"]
["Standardni pripomočki","Izpustni čep","","","","","1","1","1","1"]
["","Priročnik za namestitev","","","","","1","1","1","1"]
["","Oznaka polnitve hladilnega sredstva","","","","","1","1","","1"]
["","Večjezikovne oznake za fluorirane toplogredne pline","","","","","1","1","","1"]
["Hladilno sredstvo","Charge","","","TCO2Eq","","","2.1","2.5"]
["","GWP","","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Polnjenje","","","kg","","1.70","1.0","1.2","1.50"]
["","Tip","","","","","R-410A","R-410A","R-410A","R-410A"]
["Motor ventilatorja","Speed","Hlajenje","Izjwemno nizka","vrt/min","","","780","780"]
["","","Gretje","Izjwemno nizka","vrt/min","","","740","740"]
["Območje delovanja","Hlajenje","Okolje","Maks.","° CDB","","46","46","46","46"]
["","","","Min.","° CDB","","-10","10","10","-10"]
["","Gretje","Okolje","Maks.","° CWB","","18","18","18","18"]
["","","","Min.","° CWB","","-15","-15","-15","-15"]
["Priključki cevne napeljave","Višinska razlika","IU - OU","Maks.","m","","20.0","15","15","20.0"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)"]
["Raven zvočne moči","Hlajenje","","","dBA","","65","","","62"]
["","Gretje","","","dBA","","65","","","62"]
["Kompresor","Tip","","","","","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor"]
["Mere","Enota","","Width","mm","","825","765","765","825"]
["","","","Depth","mm","","300","285","285","300"]
["","","","Height","mm","","735","550","550","735"]
["Teža","Unit","","","kg","","47","34","34","47"]
["Ventilator","Hitrost pretoka zraka","Ogrevanje","Izjemno nizka","cfm","","","904","904"]
["","","","Izjemno nizka","m³/min","","","25.6","25.6"]
["","","Hlajenje","Izjemno nizka","m³/min","","","30.1","30.1"]
["","","","Izjemno nizka","cfm","","","1,063","1,063"]
["Power supply","Faza","","","","","1~","1~","1~","1~"]
["","Frekvenca","","","Hz","","50","50","50","50"]
["","Napetost","","","V","","220-230-240","220-240","220-240","220-230-240"]
["Opombe","","","","","(1) - 220V","","(1) - Ob priklopu na večsistemsko zunanjo enoto glejte specifikacije za multi zunanjo enoto, ki naj se priklopi.","(1) - Ob priklopu na večsistemsko zunanjo enoto glejte specifikacije za multi zunanjo enoto, ki naj se priklopi."]
["","","","","","(2) - 230V","","(2) - 220V","(2) - 220V"]
["","","","","","(3) - 240V","","(3) - 230V","(3) - 230V"]
["","","","","","","","(4) - 240V","(4) - 240V"]
["","","","","","","","(5) - Vsebuje fluorirane toplogredne pline","(5) - Vsebuje fluorirane toplogredne pline"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Izjemno nizka","m³/min","48.9"]
["","","Ogrevanje","Izjemno nizka","m³/min","43.1"]
["","","","Izjemno nizka","cfm","1727"]
["","","Ogrevanje","Izjemno nizka","cfm","1522"]
["Mere","Enota","","Višina","mm","735"]
["","","","Širina","mm","825"]
["","","","Globina","mm","300"]
["Teža","Enota","","","kg","47"]
["Motor ventilatorja","Hitrost","Hlajenje","Izjwemno nizka","vrt/min","670"]
["","","Ogrevanje","Izjwemno nizka","vrt/min","670"]
["Kompresor","Tip","","","","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","° CDB","10"]
["","","","Maks.","° CDB","46"]
["","Gretje","Okolje","Min.","° CWB","-15"]
["","","","Maks.","° CWB","18"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","48"]
["","Gretje","","Visok","dBA","48"]
["Hladilno sredstvo","Tip","","","","R-410A"]
["","Polnitev","","","kg","1.7"]
["","Polnjenje","","","tCO2Eq","3.5"]
["","GWP","","","","2087.5"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","30"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 10m)"]
["","Višinska razlika","IU - OU","Maks.","m","20"]
["Standardni pripomočki","Installation manual","","","","1"]
["","Drain plug","","","","1"]
["Napajanje","Faza","","","","1~"]
["","Frekvenca","","","Hz","50"]
["","Napetost","","","V","220-240"]
["Opombe","","","","","","(1) - Vsebuje fluorirane toplogredne pline","","","(1) - Vsebuje fluorirane toplogredne pline"]