{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L3"]
[]
[]
[]
[]
["","","","","","ARXS25L3V1B","ARXS35L3V1B"]
["Raven zvočnega tlaka","Gretje","","Visok","dBA","","48"]
["","","","Nizko","dBA","","45"]
["Standardni pripomočki","1","","","","","550"]
["Hladilno sredstvo","Polnitev","","","kg","","2.5"]
["","Tip","","","","","1.2"]
["Fan","Hitrost pretoka zraka","Hlajenje","Izjemno nizka","m³/min","","30.1"]
["","","","Izjemno nizka","cfm","","1,063"]
["Motor ventil.","Hitrost","Hlajenje","Izjwemno nizka","vrt/min","","740"]
["","","Gretje","Izjwemno nizka","vrt/min","","-15"]
["Območje delovanja","Gretje","Okolje","Min.","° CWB","","20"]
["","","","Maks.","° CWB","","10"]
["Raven zvočnega tlaka","Hlajenje","","Nizko","dBA","","44"]
["","","","Visok","dBA","","48"]
["Compressor","Type","","","","","Hermetično zaprt nihajni kompresor"]
["Mere","Enota","","Širina","mm","","285"]
["","","","Globina","mm","","612"]
["","","","Višina","mm","","765"]
["Teža","Enota","","","kg","","34"]
["Fan","Hitrost pretoka zraka","Gretje","Izjemno nizka","cfm","","904"]
["","","","Izjemno nizka","m³/min","","25.6"]
["Power supply","Phase","","","","","1~"]
["","Frekvenca","","","Hz","","50"]
["","Napetost","","","V","","220-240"]
["Opombe","","","","","(1) - 220V","(1) - Vsebuje fluorirane toplogredne pline"]
["","","","","","(2) - 230V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - 230V"]
["","","","","","","(4) - 240V"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Izjemno nizka","m³/min","30.1"]
["","","Ogrevanje","Izjemno nizka","m³/min","25.6"]
["","","","Izjemno nizka","cfm","1063"]
["","","Ogrevanje","Izjemno nizka","cfm","904"]
["Mere","Enota","","Višina","mm","550"]
["","","","Širina","mm","765"]
["","","","Globina","mm","285"]
["Teža","Enota","","","kg","34"]
["Motor ventilatorja","Hitrost","Hlajenje","Izjwemno nizka","vrt/min","780"]
["","","Ogrevanje","Izjwemno nizka","vrt/min","740"]
["Kompresor","Tip","","","","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","° CDB","10"]
["","","","Maks.","° CDB","46"]
["","Gretje","Okolje","Min.","° CWB","-15"]
["","","","Maks.","° CWB","18"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","46"]
["","Gretje","","Visok","dBA","47"]
["","","","Nizko","dBA","44"]
["Hladilno sredstvo","Tip","","","","R-410A"]
["","Polnitev","","","kg","1.0"]
["","Polnjenje","","","tCO2Eq","2.1"]
["","GWP","","","","2087.5"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","20"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 10m)"]
["","Višinska razlika","IU - OU","Maks.","m","15"]
["Standardni pripomočki","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain plug","","","","1"]
["Napajanje","Faza","","","","1~"]
["","Frekvenca","","","Hz","50"]
["","Napetost","","","V","220-240"]