{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":7,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-G"]
[]
[]
[]
[]
["","","","","","ATXF25G5V1B","ATXF35G5V1B"]
["Vhodna moč","Hlajenje","","Nom.","kW","0.023","0.029"]
["","Gretje","","Nom.","kW","0.023","0.023"]
["Ohišje","Barva","","","","Bela","Bela"]
["Mere","Enota","","Višina","mm","286","286"]
["","","","Širina","mm","770","770"]
["","","","Globina","mm","225","225"]
["Teža","Enota","","","kg","8.5","9"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","9.8","10.9"]
["","","","Srednja","m³/min","8","7"]
["","","","Nizko","m³/min","6","5.7"]
["","","","Tiho delovanje","m³/min","4.3","4.6"]
["","","Gretje","Visok","m³/min","10.4","9.3"]
["","","Ogrevanje","Srednja","m³/min","8.4","7.5"]
["","","Gretje","Nizko","m³/min","6.4","6"]
["","","","Tiho delovanje","m³/min","5.3","5.2"]
["Raven zvočne moči","Hlajenje","","","dBA","54","54"]
["","Gretje","","","dBA","55","56"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","40","56"]
["","","","Srednja","dBA","33"]
["","","","Nizko","dBA","26"]
["","","","Tiho delovanje","dBA","20"]
["","Gretje","","Visok","dBA","40","40"]
["","Ogrevanje","","Srednja","dBA","34","35"]
["","Gretje","","Nizko","dBA","28","29"]
["","","","Tiho delovanje","dBA","21","21"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","6","6"]
["","Plin","","Zun. premer","mm","9.5","9.5"]
["","Izpust","","","","18","18"]
["Krmilni sistemi","Infrardeči daljinski upravljalnik","","","","ARC480A93","ARC480A93"]
["","Ožičeni daljinski krmilnik","","","","BRC073A1","BRC073A1"]
["Standardni pripomočki","Installation manual","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Infrared remote control","","","","1","1"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Napajanje","Faza","","","","1~","1~"]
["","Frekvenca","","","Hz","50","50"]
["","Napetost","","","V","220-440","220-440"]
["Opombe","","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m"]
["","","","","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5 m (horizontalno)","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5 m (horizontalno)"]
["","","","","","(3) - Glejte ločeno risbo za električne podatke","(3) - Glejte ločeno risbo za električne podatke"]