{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":95,"n_cols":13,"rows_kept":95,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R"]
[]
[]
[]
[]
["","","","","","ATXM20R2V1B §$ ATXM20R5V1B","ATXM20R2V1B (Archived)","ATXM20R5V1B (Archived)","ATXM25R2V1B (Archived)","ATXM25R5V1B (Archived)","ATXM35R2V1B (Archived)","ATXM35R5V1B (Archived)","ATXM50R2V1B (Archived)"]
["Raven zvočnega tlaka","Gretje","","Visok","dBA","39"]
["","","","Srednja","dBA","34"]
["","","","Tiho delovanje","dBA","20"]
["","","","Nizko","dBA","26"]
["","Hlajenje","","Srednja","dBA","33"]
["","","","Tiho delovanje","dBA","19"]
["","","","Nizko","dBA","25"]
["","","","Visok","dBA","41"]
["Standardni pripomočki","Priročnik za namestitev","","","","1"]
["","Priročnik za upravljanje","","","","1"]
["","Brezžičen daljinski upravljalnik","","","","1"]
["","Suhe baterije AAA","","","","2"]
["","Držalo daljinskega upravljalnika","","","","1"]
["","Priključna plošča","","","","1"]
["","Filter iz titanovega apatita za odstranjevanje neprijetnih vonjav","","","","1"]
["","Fiksirni vijaki notranje enote","","","","2"]
["","WLAN adapterski komplet","","","","1"]
["Krmilni sistemi","Wired remote control","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A67"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","6.35"]
["","Plin","","Zun. premer","mm","9.50"]
["","priključka","","","","18"]
["Vhodna moč","Hlajenje","","Nom.","kW","0.029"]
["","Gretje","","Nom.","kW","0.023"]
["Raven zvočne moči","Hlajenje","","","dBA","58"]
["","Gretje","","","dBA","55"]
["Mere","Enota","","Širina","mm","778"]
["","","","Globina","mm","272"]
["","","","Višina","mm","295"]
["Ohišje","Barva","","","","Bela"]
["Teža","Enota","","","kg","10.0"]
["Ventilator","Hitrost pretoka zraka","Gretje","Visok","m³/min","9.3"]
["","","","Srednja","m³/min","8.2"]
["","","","Nizko","m³/min","6.2"]
["","","","Tiho delovanje","m³/min","5.1"]
["","","Hlajenje","Nizko","m³/min","5.7"]
["","","","Srednja","m³/min","7.5"]
["","","","Visok","m³/min","10.5"]
["","","","Tiho delovanje","m³/min","4.3"]
["Power supply","Faza","","","","1~"]
["","Ime","","","","V1"]
["","Frekvenca","","","Hz","50"]
["","Napetost","","","V","220-240"]
["Opombe","","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(1) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m"]
["","","","","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m","(2) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m"]
["Vhodna moč","Hlajenje","","Nom.","kW","","0.029","0.029","0.029","0.029","0.03","0.03","0.03"]
["","Gretje","","Nom.","kW","","0.023","0.023","0.022","0.022","0.027","0.027","0.032"]
["Ohišje","Barva","","","","","Bela","Bela","Bela","Bela","Bela","Bela","Bela"]
["Mere","Enota","","Višina","mm","","295","295","295","295","295","295","299"]
["","","","Širina","mm","","778","778","778","778","778","778","998"]
["","","","Globina","mm","","272","272","272","272","272","272","292"]
["Teža","Enota","","","kg","","10","10","10","10","10","10","14.5"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","","10.5","10.5","10.5","10.5","11.3","11.3","15.8"]
["","","","Srednja","m³/min","","7.5","7.5","7.6","7.6","7.8","7.8","14"]
["","","","Nizko","m³/min","","5.7","5.7","5.7","5.7","6","6","11.4"]
["","","","Tiho delovanje","m³/min","","4.3","4.3","4.1","4.1","4.2","4.2","8.3"]
["","","Gretje","Visok","m³/min","","9.3","9.3","9.8","9.8","9.8","9.8","15.8"]
["","","Ogrevanje","Srednja","m³/min","","8.2","8.2","8","8","8.5","8.5","14.2"]
["","","Gretje","Nizko","m³/min","","6.2","6.2","6.3","6.3","6.5","6.5","12"]
["","","","Tiho delovanje","m³/min","","5.1","5.1","4.9","4.9","4.9","4.9","10.5"]
["Raven zvočne moči","Hlajenje","","","dBA","","58","58","58","58","58","58","58"]
["","Gretje","","","dBA","","55","55","55","55","55","55","58"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","","41","41","41","41","45","45","44"]
["","","","Srednja","dBA","","33","33","33","33","33","33","40"]
["","","","Nizko","dBA","","25","25","25","25","25","25","36"]
["","","","Tiho delovanje","dBA","","19","19","19","19","19","19","27"]
["","Gretje","","Visok","dBA","","39","39","39","39","39","39","43"]
["","Ogrevanje","","Srednja","dBA","","34","34","34","34","35","35","39"]
["","Gretje","","Nizko","dBA","","26","26","27","27","28","28","34"]
["","","","Tiho delovanje","dBA","","20","20","20","20","20","20","31"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Plin","","Zun. premer","mm","","9.5","9.5","9.5","9.5","9.5","9.5","12.7"]
["","Izpust","","","","","18","18","18","18","18","18","18"]
["Krmilni sistemi","Infrardeči daljinski upravljalnik","","","","","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67"]
["","Ožičeni daljinski krmilnik","","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standardni pripomočki","Installation manual","","","","","1","1","1","1","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","","2","2","2","2","2","2","2"]
["","WLAN adapter kit","","","","","1","1","1","1","1","1","1"]
["","Operation manual","","","","","1","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","1","1","1","1","1","1","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","1","1"]
["Napajanje","Ime","","","","","V1","V1","V1","V1","V1","V1","V1"]
["","Faza","","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frekvenca","","","Hz","","50","50","50","50","50","50","50"]
["","Napetost","","","V","","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standardni pripomočki","Silver particle filter","","","","","","","","","","","1"]