{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":8,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-N9"]
[]
[]
[]
[]
["","","","","","ATXP20N5V1B9","ATXP25N5V1B9","ATXP35N5V1B9"]
["Vhodna moč","Hlajenje","","Nom.","kW","0.019","0.020","0.032"]
["","Gretje","","Nom.","kW","0.023","0.023","0.032"]
["Ohišje","Barva","","","","Bela","Bela","Bela"]
["Mere","Enota","","Višina","mm","286","286","286"]
["","","","Širina","mm","770","770","770"]
["","","","Globina","mm","225","225","225"]
["Teža","Enota","","","kg","8.50","8.50","9.00"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","9.5","9.7","11.5"]
["","","","Medium","m³/min","7.4","7.7","8.3"]
["","","","Nizko","m³/min","5.6","5.8","6.3"]
["","","","Tiho delovanje","m³/min","4.2","4.2","4.5"]
["","","Gretje","Visok","m³/min","10.4","10.4","11.5"]
["","","","Medium","m³/min","8.1","8.1","9.0"]
["","","","Nizko","m³/min","6.2","6.4","7.0"]
["","","","Tiho delovanje","m³/min","5.2","5.2","5.1"]
["Raven zvočne moči","Hlajenje","","","dBA","55","55","58"]
["","Gretje","","","dBA","55","55","58"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","39","40","43"]
["","","","Medium","dBA","33","33","34"]
["","","","Nizko","dBA","25","26","27"]
["","","","Tiho delovanje","dBA","19","19","20"]
["","Gretje","","Visok","dBA","39","40","40"]
["","","","Srednja","dBA","34","34","35"]
["","","","Nizko","dBA","28","28","29"]
["","","","Tiho delovanje","dBA","21","21","21"]
["Priključki napeljave","Tekočina","","Zun. premer","mm","6","6","6"]
["","Gas","","OD","mm","9.50","9.50","9.50"]
["","priključka","","","","18","18","18"]
["Krmilni sistemi","Infrared remote control","","","","ARC480A78","ARC480A78","ARC480A78"]
["","Wired remote control","","","","BRC073A1","BRC073A1","BRC073A1"]
["Standardni pripomočki","Priročnik za namestitev","","","","1","1","1"]
["","Priročnik za upravljanje","","","","1","1","1"]
["","Infrardeči daljinski upravljalnik","","","","1","1","1"]
["","Suhe baterije AAA","","","","2","2","2"]
["","Držalo daljinskega upravljalnika","","","","1","1","1"]
["","Priključna plošča","","","","1","1","1"]
["","Filter iz titanovega apatita za odstranjevanje neprijetnih vonjav","","","","1","1","1"]
["","Filter srebrnih delcev","","","","1","1","1"]
["","Fiksirni vijaki notranje enote","","","","2","2","2"]
["","Splošni varnostni previdnostni ukrepi","","","","1","1","1"]
["Power supply","Faza","","","","1~","1~","1~"]
["","Frekvenca","","","Hz","50","50","50"]
["","Napetost","","","V","220-240","220-240","220-240"]
["Opombe","","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m"]
["","","","","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5 m (horizontalno)","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5 m (horizontalno)","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5 m (horizontalno)"]
["","","","","","(3) - Glejte ločeno risbo za električne podatke","(3) - Glejte ločeno risbo za električne podatke","(3) - Glejte ločeno risbo za električne podatke"]