{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":8,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AZAS-MY1"]
[]
[]
[]
[]
["","","","","","AZAS100M7Y1B","AZAS125M7Y1B","AZAS140M7Y1B"]
["Mere","Enota","","Višina","mm","990","990","990"]
["","","","Širina","mm","940","940","940"]
["","","","Globina","mm","320","320","320"]
["Teža","Enota","","","kg","","70"]
["Kompresor","Tip","","","","","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","°CDB","-5","-5","-5"]
["","","","Maks.","°CDB","46","46","46"]
["","Gretje","Okolje","Min.","° CWB","-15","-15","-15"]
["","","","Maks.","° CWB","15.5","15.5","15.5"]
["Raven zvočne moči","Hlajenje","","","dBA","70","71","73"]
["","Gretje","","","dBA","","71","73 (1)"]
["Raven zvočnega tlaka","Hlajenje","","Nom.","dBA","53","53","54"]
["","Gretje","","Nom.","dBA","57","57","57"]
["Hladilno sredstvo","Tip","","","","R-32","R-32","R-32"]
["","Hladilno sredstvo-=-Polnjenje-=-kg","","","kg","","2.60"]
["Hladilno sredstvo","GWP","","","","","675"]
["Hladilno sredstvo","Polnjenje","","","tCO2Eq","1.76","1.76","1.96"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","9.52","9.52","9.52"]
["Priključki cevne napeljave","Plin","","Zun. premer","mm","","15.9"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","30","30","30"]
["","","Sistem","Ekvivalent","m","50","50","50"]
["","","","Brez polnitve","m","30","30","30"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","Glejte priročnik za namestitev","Glejte priročnik za namestitev","Glejte priročnik za namestitev"]
["","Višinska razlika","IU - OU","Maks.","m","30.0","30.0","30.0"]
["","","IU - IU","Maks.","m","0.5","0.5","0.5"]
["Standardni pripomočki","Installation manual","","","","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Tie-wraps","","","","2","2","2"]
["Napajanje","Faza","","","","3~","3~","3~"]
["","Napajanje-=-Frekvenca","","Frekvenca","","50","50","50"]
["","Napajanje-=-Napetost","","Napetost","","380-415","380-415","380-415"]
["Tok - 50 Hz","Tok - 50 Hz-=-Maksimalni tok varovalk (MFA)","","Tok - 50 Hz-=-Maksimalni tok varovalk (MFA)-=-A","","","16"]
["Opombe","","","","","","(1) - V skladu z ENER Lot 21","(1) - V skladu z ENER Lot 21"]
["Teža","Enota","","","kg","70","","77"]
["Kompresor","Tip","","","","Hermetično zaprt nihajni kompresor","","Hermetično zaprt nihajni kompresor"]
["Hladilno sredstvo","Polnitev","","","kg","2.60","","2.90"]
["","GWP","","","","675","","675"]
["Priključki cevne napeljave","Plin","","Zun. premer","mm","15.9","","15.9"]
["Tok – 50 Hz","Maksimalni tok varovalk (MFA)","","","A","16","","16"]