{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BR00000678"]
[]
[]
[]
[]
["","","","","","BR00000678."]
["Uporaba","","","","","Samostoječi tip"]
["Kapaciteta","m³/min","","","","33.33"]
["Ohišje","Barva","","","","Prebarvana galvanizirana jeklena plošča"]
["Mere","Enota","","Višina","mm","1628"]
["","","","Širina","mm","720"]
["","","","Globina","mm","770"]
["Teža","Enota","","","kg","150"]
["Ustrezna površina prostora","m²","","","","133"]
["Delovanje za čiščenje zraka","Vhodna moč","","H","kW","0.379"]
["Raven zvočnega tlaka","Delovanje za čiščenje zraka","","Visok","dBA","55.9"]
["Ventilator","Hitrost pretoka zraka","Delovanje za čiščenje zraka","Turbo","m³/h","2300"]
["","","","Visok","m³/h","2000"]
["Varnostne naprave","Postavka","","01","","Varnostno stikalo (delovanje se ustavi, ko se odprejo zadnja vrata)"]
["Standardni pripomočki","Prefilter selected","","","","1"]
["","HEPA filter selected","","","","1"]
["","Quick Start and Maintenance Guide","","","","1"]
["","Installation and Operation Manual available for download","","","","1"]
["Napajalni kabel","m","","","","3"]
["Napajanje","Frekvenca","","","Hz","50/60"]
["Obratovalni tok","Delovanje za čiščenje zraka","","Visok","A","1.73"]