{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1H52W"]
[]
[]
[]
[]
["","","","","BRC1H52W."]
["Embalaža","Material","","","Karton"]
["","Teža","","kg","0.0850"]
["Temperatura okolice","Relativna vlažnost <","","%","95"]
["","Skladiščenje","Min.","°C","-20"]
["","","Maks.","°C","70"]
["","Delovanje","Min.","°C","-10"]
["","","Maks.","°C","50"]
["Mere","Enota v embalaži","Širina","mm","217"]
["","","Višina","mm","50"]
["","","Globina","mm","161"]
["","Enota","Širina","mm","85"]
["","","Globina","mm","25"]
["","","Višina","mm","85"]
["Ohišje","Spodnji pokrov","","","ne"]
["","Barva","","","Bela"]
["","LED za obratovanje","Barva","","Blue status indicator"]
["LCD","Tip","","","100 x 150 dots"]
["","Zadnja luč","Barva","","Bela"]
["","Mere","Širina","mm","28.0"]
["","","Višina","mm","40.7"]
["Teža","Enota v embalaži","","kg","0.317"]
["","Enota","","kg","0.110"]
["Priključki za napeljavo","Dolžina napeljave","Maks.","m","500"]