{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CB"]
[]
[]
[]
[]
["","CB124_UK_403789","CB124_EU_403765"]
["Opombe","(1) - Rezultati energijskega testiranja so navedeni za podnebni razred 3, postopek testiranja v skladu s standardom EN 23953-2, uporaba nočne zatemnitve v trajanju 12 ur, razsvetljava vključena 12 ur","(1) - Rezultati energijskega testiranja so navedeni za podnebni razred 3, postopek testiranja v skladu s standardom EN 23953-2, uporaba nočne zatemnitve v trajanju 12 ur, razsvetljava vključena 12 ur"]
["Opombe","(2) - S procesom povezano notranjo opremo","(2) - S procesom povezano notranjo opremo"]