{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32"]
[]
[]
[]
[]
["","","","","","CHYHBH05AAV32","CHYHBH05AFV32","CHYHBH08AFV32"]
["Ohišje","Barva","","","","Bela","Bela","Bela"]
["","Material","","","","Vnaprej premazana pločevina","Vnaprej premazana pločevina","Vnaprej premazana pločevina"]
["Mere","Enota","","Višina","mm","902","902","902"]
["","","","Širina","mm","450","450","450"]
["","","","Globina","mm","164","164","164"]
["Teža","Enota","","","kg","30.0","30.0","30.0"]
["PED","Kategorija","","","","","Art3§3, Izključeno iz obsega PED po členu 1, postavka 3.6  v okviru 97/23/EC","Art3§3, Izključeno iz obsega PED po členu 1, postavka 3.6  v okviru 97/23/EC"]
["Toplotni izmenjevalnik na strani vode","Hitrost pretoka vode","Ogrevanje","Maks.","l/min","23.0 (5)","23.0 (5)","23.0 (5)"]
["Raven zvočne moči","Nom.","","","dBA","42 (6)","42 (6)","42 (6)"]
["Območje delovanja","Gretje","Stran vode","Min.","° C","25 (7)","25 (7)","25 (7)"]
["","","","Maks.","° C","50 (7)","50 (7)","50 (7)"]
["Napajanje","Ime","","","","V3","V3","V3"]
["","Faza","","","","1~","1~","1~"]
["","Frekvenca","","","Hz","50","50","50"]
["","Napetost","","","V","230","230","230"]
["Priključki za napeljavo","Za priključitev na uporabniški vmesnik","","Količina","","2","2","2"]
["","","","Opomba","","0,75 mm² do 1,25 mm² (maks. dolžina 500 m)","0,75 mm² do 1,25 mm² (maks. dolžina 500 m)","0,75 mm² do 1,25 mm² (maks. dolžina 500 m)"]
["Opombe","","","","","(1) - Samo za notranjo enoto","(1) - Samo za notranjo enoto","(1) - Samo za notranjo enoto"]
["","","","","","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), obvod grelnika","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), obvod grelnika","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), obvod grelnika"]
["","","","","","(3) - DB/WB 7°C/6°C - LWC 45℃ (DT=5°C), obvod grelnika","(3) - DB/WB 7°C/6°C - LWC 45℃ (DT=5°C), obvod grelnika","(3) - DB/WB 7°C/6°C - LWC 45℃ (DT=5°C), obvod grelnika"]
["","","","","","(4) - Min. required","(4) - Min. required","(4) - Min. required"]
["","","","","","(5) - Obvod grelnika","(5) - Obvod grelnika","(5) - Obvod grelnika"]
["","","","","","(6) - V skladu z EN14825","(6) - V skladu z EN14825","(6) - V skladu z EN14825"]
["","","","","","(7) - Za obratovalni doseg *HYHB* in *HYKOMB33AA glejte shemo obratovalmega dosega","(7) - Za obratovalni doseg *HYHB* in *HYKOMB33AA glejte shemo obratovalmega dosega","(7) - Za obratovalni doseg *HYHB* in *HYKOMB33AA glejte shemo obratovalmega dosega"]