{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-AT"]
[]
[]
[]
[]
["","","","","CTXA15A2V1BT"]
["Raven zvočnega tlaka","Gretje","Visok","dBA","39"]
["","","Srednja","dBA","32"]
["","","Tiho delovanje","dBA","21"]
["","","Nizko","dBA","25"]
["","Hlajenje","Srednja","dBA","32"]
["","","Tiho delovanje","dBA","21"]
["","","Nizko","dBA","25"]
["","","Visok","dBA","39"]
["Standardni pripomočki","Priročnik za namestitev","","","1"]
["","Priročnik za upravljanje","","","1"]
["","Zračni filter","","","2"]
["","Infrardeči daljinski upravljalnik","","","1"]
["","Montirna plošča daljinskega upravljalnika","","","1"]
["","Vrečka vijaka","","","1"]
["","Vijačni pokrov","","","1"]
["","Suhe baterije AAA","","","2"]
["","Splošni varnostni previdnostni ukrepi","","","1"]
["Hladilno sredstvo","GWP","","","675.0"]
["Krmilni sistemi","Wired remote control","","","BRC073"]
["","Infrared remote control","","","ARC466A58"]
["Priključki cevne napeljave","Tekočina","Zun. premer","mm","6.35"]
["","Plin","Zun. premer","mm","9.50"]
["","priključka","","","18"]
["Vhodna moč","Hlajenje","Nom.","kW","0.020"]
["","Gretje","Nom.","kW","0.020"]
["Raven zvočne moči","Hlajenje","","dBA","57"]
["Mere","Enota","Širina","mm","798"]
["","","Globina","mm","189"]
["","","Višina","mm","295"]
["Ohišje","Barva","","","Črn les"]
["Teža","Enota","","kg","12"]
["Power supply","Faza","","","1~"]
["","Frekvenca","","Hz","50"]
["","Ime","","","V1"]
["","Napetost","","V","220-240"]