{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R / 5MXM-N9"]
[]
[]
[]
[]
["","","","","CTXM15R2V1B / FTXM71R2V1B / 5MXM90N2V1B9","CTXM15R5V1B / FTXM71R2V1B / 5MXM90N2V1B9"]
["Hladilna kapaciteta","Nom.","","kW","8.00","8.00"]
["Hlajenje prostora","SEER","","","6.84","6.84"]
["","Letna poraba energije","","kWh/a","410","410"]
["","Zmogljivost","Pdizajn","kW","8.00","8.00"]
["","Razred energijske učinkovitosti","","","A+++","A+++"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","4.50","4.50"]
["","SCOP/A","","","4.28","4.28"]
["","Razred energijske učinkovitosti","","","A+","A+"]
["","Letna poraba energije","","kWh/a","1,472","1,472"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","1,202","1,202"]
["","EER","","","3.33","3.33"]
["","COP","","","3.67","3.67"]
["","Direktiva o energijskih oznakah","Hlajenje","","A","A"]
["","","Ogrevanje","","A","A"]
["Grelna kapaciteta","Nom.","","kW","10.00","10.00"]
["Opombe","","","","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m"]
["","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]
["","","","","(3) - Glejte ločeno risbo za obratovalno območje","(3) - Glejte ločeno risbo za obratovalno območje"]
["","","","","(4) - Glejte ločeno risbo za električne podatke","(4) - Glejte ločeno risbo za električne podatke"]