{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":9,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Raven zvočnega tlaka","Gretje","","Visok","dBA","38","","41"]
["","","","Tiho delovanje","dBA","21","","21"]
["","","","Nizko","dBA","28","","30"]
["","Hlajenje","","Tiho delovanje","dBA","21","","21"]
["","","","Nizko","dBA","25","","28"]
["","","","Visok","dBA","37","","42"]
["","","","Nom.","dBA","33"]
["","Hlajenje","","Nom.","dBA","31","","35"]
["Standardni pripomočki","Priročnik za namestitev","","","","1","","1"]
["","Priročnik za upravljanje","","","","1","","1"]
["","Brezžičen daljinski upravljalnik","","","","1","","1"]
["","Baterije","","","","2","","2"]
["","Držalo daljinskega upravljalnika","","","","1","","1"]
["","Priključna plošča","","","","1","","1"]
["","Fiksirni vijaki notranje enote","","","","2","","2"]
["","Fotokatalizatorski filter iz titanovega apatita za čiščenje zraka","","","","2","","2"]
["Krmilni sistemi","Infrared remote control","","","","ARC466A6","","ARC466A6"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","6.35","","6.35"]
["","Plin","","Zun. premer","mm","9.5","","9.5"]
["","Izpust","","","","18","","18"]
["Vhodna moč","Hlajenje","","Nom.","kW","0.040","","0.040"]
["","Gretje","","Nom.","kW","0.040","","0.040"]
["Raven zvočne moči","Hlajenje","","","dBA","55","","59"]
["","Gretje","","","dBA","56","","58"]
["Mere","Enota","","Širina","mm","780","","780"]
["","","","Globina","mm","215","","215"]
["","","","Višina","mm","289","","289"]
["Ohišje","Barva","","","","Bela","","Bela"]
["Teža","Enota","","","kg","8","","8"]
["Ventilator","Hitrost pretoka zraka","Gretje","Visok","m³/min","","","10.1"]
["","","","Nizko","m³/min","","","6.3"]
["","","","Tiho delovanje","m³/min","","","4.3"]
["","","Hlajenje","Nizko","m³/min","","","5.2"]
["","","","Visok","m³/min","","","9.2"]
["","","","Tiho delovanje","m³/min","","","3.9"]
["","","","Nom.","m³/min","","","8.1"]
["","","Hlajenje","Nom.","m³/min","","","7.2"]
["Power supply","Faza","","","","1~","","1~"]
["","Frekvenca","","","Hz","50","","50"]
["","Ime","","","","V1","","V1"]
["","Napetost","","","V","220-240","","220-240"]
["Opombe","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Vhodna moč","Hlajenje","","Nom.","kW","","0.04","","0.040"]
["","Gretje","","Nom.","kW","","0.04","","0.040"]
["Ohišje","Barva","","","","","Bela","","Bela"]
["Mere","Enota","","Višina","mm","","289","","289"]
["","","","Širina","mm","","780","","780"]
["","","","Globina","mm","","215","","215"]
["Teža","Enota","","","kg","","8","","8.00"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","","7.9","","9.2"]
["","","","Srednja","m³/min","","6.3","","7.2"]
["","","","Nizko","m³/min","","4.7","","5.2"]
["","","","Tiho delovanje","m³/min","","3.9","","3.9"]
["","","Gretje","Visok","m³/min","","9","","10.1"]
["","","Ogrevanje","Srednja","m³/min","","7.5","","8.1"]
["","","Gretje","Nizko","m³/min","","6","","6.3"]
["","","","Tiho delovanje","m³/min","","4.3","","4.3"]
["Raven zvočne moči","Hlajenje","","","dBA","","55","","59"]
["","Gretje","","","dBA","","56","","58"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","","37","","42"]
["","","","Srednja","dBA","","31","","35"]
["","","","Nizko","dBA","","25","","28"]
["","","","Tiho delovanje","dBA","","21","","21"]
["","Gretje","","Visok","dBA","","38","","41"]
["","Ogrevanje","","Srednja","dBA","","33","","36"]
["","Gretje","","Nizko","dBA","","28","","30"]
["","","","Tiho delovanje","dBA","","21","","21"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","","6.35","","6.35"]
["","Plin","","Zun. premer","mm","","9.5","","9.50"]
["","Izpust","","","","","18","","18"]
["Krmilni sistemi","Infrared remote control","","","","","ARC466A6","","ARC466A6"]
["Standardni pripomočki","Installation manual","","","","","1","","1"]
["","Wireless remote control","","","","","1","","1"]
["","AAA dry-cell batteries","","","","","2","","2"]
["","Operation manual","","","","","1","","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2"]
["","Indoor unit fixing screws","","","","","2","","2"]
["","Mounting plate","","","","","1","","1"]
["","Remote control holder","","","","","1","","1"]
["Napajanje","Ime","","","","","V1","","V1"]
["","Faza","","","","","1~","","1~"]
["","Frekvenca","","","Hz","","50","","50"]
["","Napetost","","","V","","220-240","","220-240"]