{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CVXM-A9"]
[]
[]
[]
[]
["","","","","","CVXM20A3V1B9"]
["Vhodna moč","Hlajenje","","Nom.","kW","0.02"]
["","Gretje","","Nom.","kW","0.02"]
["Ohišje","Barva","","","","Bela"]
["Mere","Enota","","Višina","mm","600"]
["","","","Širina","mm","750"]
["","","","Globina","mm","238"]
["Teža","Enota","","","kg","17"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","8.7"]
["","","","Srednja","m³/min","7"]
["","","","Nizko","m³/min","4.9"]
["","","","Tiho delovanje","m³/min","4.1"]
["","","Gretje","Visok","m³/min","9.2"]
["","","Ogrevanje","Srednja","m³/min","7.2"]
["","","Gretje","Nizko","m³/min","5.6"]
["","","","Tiho delovanje","m³/min","4.1"]
["Raven zvočne moči","Hlajenje","","","dBA","52"]
["","Gretje","","","dBA","52"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","38"]
["","","","Srednja","dBA","32"]
["","","","Nizko","dBA","25"]
["","","","Tiho delovanje","dBA","22"]
["","Gretje","","Visok","dBA","38"]
["","Ogrevanje","","Srednja","dBA","32"]
["","Gretje","","Nizko","dBA","25"]
["","","","Tiho delovanje","dBA","21"]
["Hladilno sredstvo","GWP","","","","675"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","6.4"]
["","Plin","","Zun. premer","mm","9.5"]
["","Izpust","","","","VP20 (I.D. 20/O.D. 26)"]
["Krmilni sist.","Infrared remote control","","","","ARC466A66"]
["Krmilni sistemi","Ožičeni daljinski krmilnik","","","","BRC073A1"]
["Standardni pripomočki","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Napajanje","Faza","","","","1~"]
["","Frekvenca","","","Hz","50"]
["","Napetost","","","V","220-240"]