{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCC601A51"]
[]
[]
[]
[]
["","","","","","DCC601A51."]
["Vhodna moč","kW","","","","0.015"]
["Maksimalno število povezljivih notranjih enot","","","","","32"]
["Maksimalno število povezljivih zunanjih enot @","","","","","7"]
["Mere","Enota","","Višina","mm","136"]
["","","","Širina","mm","384"]
["","","","Globina","mm","92"]
["Komunikacije","DIII-NET","","Količina","","1"]
["","","","Opomba","","DIII-NET (F1F2)"]
["","Ethernet","","Komunikacije-=-Ethernet-=-Količina","","1"]
["","Vhodni terminal","Digitalno","Količina","","4"]
["Temperatura okolice","Delovanje","","Min.","°C","-10"]
["","","","Maks.","°C","50"]
["","Skladiščenje","","Min.","°C","-20"]
["","","","Maks.","°C","60"]
["","Temperatura okolice-=-Relativna vlažnost <-=-%","","","%","85"]
["Napajanje","Frekvenca","","","Hz","50/60"]
["","Napetost","","","V","110-240 AC"]
["Opombe","","","","","(1) - Vključuje dovod energije z WAGO izvora energije, CPU modul in I/O modul"]
["","","","","","(2) - Mere vključujejo WAGO izvor energije, CPU modul, I/O modul in potreben prostorski razmak med posameznimi deli"]
["","","","","","(3) - Mere izbirnega zaslona so: višina: 209 mm, širina: 123 mm, globina: 8,5 mm"]