{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCS601C51"]
[]
[]
[]
[]
["","","","","","DCS601C51."]
["Vhod","Tip","","","","Zaslon na dotik (10 bitno kodiran analogni vhod)"]
["Temperatura okolice","Relativna vlažnost <","","","%","85"]
["","Delovanje","","Min.","°C","0"]
["","","","Maks.","°C","40"]
["Maksimalno število povezljivih notranjih enot","","","","","64, 128 (1)"]
["Komunikacija","DIII-NET","","Količina","","1"]
["","","","Opomba","","Komunikacijski vod klimatske opreme"]
["","10BASE-T","","Opomba","","Možnost spleta"]
["","Ethernet","","Opomba","","Vhod za dostop do spleta in e-pošte"]
["","Vhodni terminal","Digitalno","Količina","","1"]
["","","","Opomba","","Prisiljena zaustavitev"]
["","","Pulzno","Količina","","3"]
["","","","Opomba","","Pulz za merjenje moči"]
["","Modem","","Opomba","","Zmožnost vgrajenega modema"]
["","PCMCIA","","Opomba","","Pomnilniška kartica flash"]
["","RS-232C","","Opomba","","Adapter DIII-NET PLUS"]
["Mere","Enota","","Širina","mm","230"]
["","","","Globina","mm","107"]
["","","","Višina","mm","147"]
["LCD","Tip","","","","QVGA (320 x 240), 4.096 barv"]
["","Mere","","Širina","palcev","5.7"]
["Maksimalno število povezljivih zunanjih enot","","","","","10, 20 (1)"]
["Power supply","Frekvenca","","","Hz","50/60"]
["","Napetost","","","V","100-240 (zunanji dovod)"]
["Opombe","","","","","(1) - V kombinaciji z DCS601A51"]