{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSHB-D3"]
[]
[]
[]
[]
["","","","","","EHSHB04P30DA3","EHSHB08P30DA3","EHSHB08P50DA3"]
["Ohišje","Barva","","","","Bela (RAL9016) / Temno siva (RAL7011)","Bela (RAL9016) / Temno siva (RAL7011)","Bela (RAL9016) / Temno siva (RAL7011)"]
["","Material","","","","Na udarec odporen polipropilen","Na udarec odporen polipropilen","Na udarec odporen polipropilen"]
["Mere","Enota","","Višina","mm","1891","1891","1896"]
["","","","Širina","mm","595","595","790"]
["","","","Globina","mm","615","615","790"]
["Teža","Enota","","","kg","76.0","76.0","99.0"]
["PED","Kategorija","","","","čl. 3.3","čl. 3.3","čl. 3.3"]
["Hladilno sredstvo","Tip","","","","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0"]
["","Polnitev","","","kg","1.50","1.50","1.50"]
["Raven zvočne moči","Nom.","","","dBA","39","39","39"]
["Območje delovanja","Gretje","Stran vode","Min.","°C","18","18","18"]
["","","","Maks.","°C","65","65","65"]
["","Hlajenje","Okolje","Min.","°CDB","10","10","10"]
["","","Stran vode","Min.","°C","5","5","5"]
["","","","Maks.","°C","22","22","22"]
["Napajanje","Faza","","","","1~","1~","1~"]
["","Frekvenca","","","Hz","50","50","50"]
["","Napetost","","","V","230","230","230"]
["Električni grelnik","Napajanje","","Ime","","3V / 9W","3V / 9W","3V / 9W"]
["","","","Faza","","1~ / 3~","1~ / 3~","1~ / 3~"]
["","","","Frekvenca","Hz","50","50","50"]
["Opombe","","","","","(1) - Toplotna izguba v skladu z EN12897","(1) - Toplotna izguba v skladu z EN12897","(1) - Toplotna izguba v skladu z EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]
["","","","","","","","(5) - Segrevanje zbiralnika samo s topl. črpalko, brez elektr. grelnika"]