{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVX-E6VG / ERGA-EV7"]
[]
[]
[]
[]
["","","","","","EHVX04S18EA6VG / ERGA04EAV37","EHVX04S23EA6VG / ERGA04EAV37"]
["Grelna kapaciteta","Nom.","","","kW","4.36, 4.60","4.36, 4.60"]
["Hladilna kapaciteta","Nom.","","","kW","4.86, 4.52","4.86, 4.52"]
["Vhodna moč","Gretje","","Nom.","kW","0.830, 1.26","0.830, 1.26"]
["","Hlajenje","","Nom.","kW","0.810, 1.36","0.810, 1.36"]
["","Segrevanje gospodinjske vode od 10°C do 50°C","","Naz.","kWh","2.48","3.01"]
["Čas segrevanja od 10°C do 50°C","ure","","","","1h 28 min","1h 40 min"]
["COP","","","","","5.23, 3.65","5.23, 3.65"]
["EER","","","","","5.98, 3.32","5.98, 3.32"]
["Gretje sanitarne tople vode","Splošno","","Profil deklarirane obremenitve","","L","XL"]
["","Povprečno podnebje","","Razred energijske učinkovitosti gretje vode","","A","A"]
["Ogrevanje prostora","Izhod vode v povprečnem podnebju 55°C","Splošno","SCOP","","3.29","3.29"]
["","","","Razred učinkovitosti sezonskega ogrevanja prostora","","A++","A++"]
["","Izhod vode v povprečnem podnebju 35°C","Splošno","SCOP","","4.96","4.96"]
["","","","Razred učinkovitosti sezonskega ogrevanja prostora","","A+++","A+++"]
["Razpon energetske učinkovitosti","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Opombe","","","","","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - 2. pogoj: hlajenje Ta 35 °C - LWE 7 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - 2. pogoj: hlajenje Ta 35 °C - LWE 7 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 45 °C (DT = 5 °C)"]