{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":9,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVZ-E6V / ERGA-EVH"]
[]
[]
[]
[]
["","","","","","EHVZ08S18EA6V / ERGA06EAV3H","EHVZ08S18EJ6V / ERGA06EAV3H","EHVZ08S23EA6V / ERGA06EAV3H","EHVZ08S23EJ6V / ERGA06EAV3H"]
["Grelna kapaciteta","Nom.","","","kW","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)"]
["Vhodna moč","Gretje","","Nom.","kW","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)"]
["","Segrevanje gospodinjske vode od 10°C do 50°C","","Naz.","kWh","2.48","2.48","3.01","3.01"]
["Čas segrevanja od 10°C do 50°C","ure","","","","1h 28 min","1h 28 min","1h 40 min","1h 40 min"]
["COP","","","","","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)"]
["Gretje sanitarne tople vode","Splošno","","Profil deklarirane obremenitve","","L","L","XL","XL"]
["","Povprečno podnebje","","Razred energijske učinkovitosti gretje vode","","A+","A+","A+","A+"]
["Ogrevanje prostora","Izhod vode v povprečnem podnebju 55°C","Splošno","SCOP","","3.26","3.26","3.26","3.26"]
["","","","Razred učinkovitosti sezonskega ogrevanja prostora","","A++","A++","A++","A++"]
["","Izhod vode v povprečnem podnebju 35°C","Splošno","SCOP","","4.47","4.47","4.47","4.47"]
["","","","Razred učinkovitosti sezonskega ogrevanja prostora","","A+++","A+++","A+++","A+++"]
["Razpon energetske učinkovitosti","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Opombe","","","","","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - 2. pogoj: hlajenje Ta 35 °C - LWE 7 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - 2. pogoj: hlajenje Ta 35 °C - LWE 7 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - 2. pogoj: hlajenje Ta 35 °C - LWE 7 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - 2. pogoj: hlajenje Ta 35 °C - LWE 7 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 45 °C (DT = 5 °C)"]