{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":6,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYKOMB-AA3"]
[]
[]
[]
[]
["","","","","","EHYKOMB33AA3"]
["Plin","Priključek","","Premer","mm","15"]
["","Poraba (G20)","","Min.","m³/h","0.79"]
["","","","Maks.","m³/h","3.39"]
["","Poraba (G25)","","Min.","m³/h","0.89"]
["","","","Maks.","m³/h","3.92"]
["","Poraba (G31)","","Min.","m³/h","0.30"]
["","","","Maks.","m³/h","1.29"]
["","NOx razred","","","","6"]
["","Raven NOx (G20)","","","mg/kWh","36"]
["Centralno ogrevanje","Vnos toplote Qn (neto kalorična vrednost)","Nom.","Min.","kW","7.6"]
["","","","Maks.","kW","27.0"]
["","Vnos toplote Qn (bruto kalorična vrednost)","Nom.","Min.","kW","8.4"]
["","","","Maks.","kW","30.0"]
["","Izhodna moč Pn pri 80/60°C","","Min.","kW","7.5"]
["","","","Nom.","kW","26.6"]
["","Izhodna moč pri 37/30°C","","Nom.","kW","8.2"]
["","Temperatura vode","","Maks.","°C","90"]
["Sanitarna topla voda","Vnos toplote (neto kalorična vrednost) Qnw","Nom.","Min.","kW","7.6"]
["","","","Maks.","kW","32.7"]
["","Vnos toplote (bruto kalorična vrednost) Qnw","Nom.","Min.","kW","8.4"]
["","","","Maks.","kW","36.3"]
["","Comfort class (EN13203)","","","","XL"]
["","Temperatura","","Maks.","°C","65"]
["Oskrbovalni zrak","Koncentrični","","","","Ne"]
["Dimni plini","Temperatura","","Maks.","°C","70"]
["","Priključitev","","","mm","60"]
["","Masni tok (G20)","","Maks.","kg/h","54.4"]
["","Masni tok (G25)","","Maks.","kg/h","54.4"]
["","Masni tok (G31)","","Maks.","kg/h","53.6"]
["Ohišje","Barva","","","","RAL9010"]
["","Material","","","","Vnaprej premazana pločevina"]
["Mere","Enota","Višina","Ohišje","mm","710"]
["","","","Širina","mm","450"]
["","","","Globina","mm","240"]
["Teža","Enota","","Prazno","kg","36"]
["Gretje sanitarne tople vode","Splošno","","Profil deklarirane obremenitve","","XL"]
["","","","Razred energijske učinkovitosti gretje vode","","A"]
["Gretje prostora","Splošno","","Razred sezonske učinkovitosti gretja prostora","","A"]