{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWC-B"]
[]
[]
[]
[]
["","","","","","EKHWC500BA"]
["Montaža","","","","","Tla"]
["Ohišje","Barva","","","","Bela (RAL9016) / Temno siva (RAL7011)"]
["","Material","","","","Na udarec odporen polipropilen"]
["Mere","Enota","Višina","Rezervoar","mm","1,660"]
["","","","Širina","mm","790"]
["","","","Globina","mm","790"]
["Teža","Enota","","Prazno","kg","69"]
["","","","Polno","kg","569"]
["Rezervoar","Volumen vode","","","l","477"]
["","Material","","","","Polipropilen"]
["","Maksimalna temperatura vode","","","°C","85"]
["","Razred energijske učinkovitosti","","","","B"]
["Toplotni izmenjevalnik","Vroča voda","","Količina","","1"]
["","","","Material cevi","","Nerjavno jeklo (DIN 1,4404)"]
["","","","Notranji volumen tuljave","l","23.8"]
["","","","Obratovalni tlak","bar","6"]
["","","","Povprečna specifična izhodna toplota","W/K","2,450"]
["","Pomožno sončno gretje","","Količina","","1"]
["","","","Material cevi","","Nerjavno jeklo (DIN 1,4404)"]
["","","","Notranji volumen tuljave","l","4"]
["","","","Obratovalni tlak","bar","3"]
["","","","Povprečna specifična izhodna toplota","W/K","350"]
["Opombe","","","","","(1) - Toplotna izguba v skladu z EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]
["","","","","","(5) - Za količino vode iz vodovodne napeljave 140 l -> 5820 Wh (kopalnica) / 8 kW toplotna črpalka"]
["","","","","","(6) - Za količino vode iz vodovodne napeljave 90 l -> 3660 Wh (kopalnica) / 8 kW toplotna črpalka"]
["","","","","","(7) - Za količino vode iz vodovodne napeljave 140 l -> 5820 Wh (kopalnica) / 16 kW toplotna črpalka"]
["","","","","","(8) - Za količino vode iz vodovodne napeljave 90 l -> 3660 Wh (kopalnica) / 16 kW toplotna črpalka"]