{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":7,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWET-BV3"]
[]
[]
[]
[]
["","","","","","EKHWET90BAV3","EKHWET120BAV3"]
["Montaža","","","","","Zid","Zid"]
["Ohišje","Barva","","","","Bela + Črna","Bela + Črna"]
["","Material","","","","Galvanizirana pločevina, Akrilonitril butadien stiren","Galvanizirana pločevina, Akrilonitril butadien stiren"]
["Mere","Enota","Višina","Rezervoar","mm","1032","1283"]
["","","","Širina","mm","510","510"]
["","","","Globina","mm","570","570"]
["Teža","Enota","","Prazno","kg","43","47"]
["Rezervoar","Volumen vode","","","l","89","118"]
["","Material","","","","Emajlirano jeklo po DIN4753TL2","Emajlirano jeklo po DIN4753TL2"]
["","Maksimalna temperatura vode","","","°C","75.0","75.0"]
["","Razred energijske učinkovitosti","","","","B","C"]
["Toplotni izmenjevalnik","Vroča voda","","Količina","","1","1"]
["","","","Material cevi","","Aluminij","Aluminij"]
["","","","Obratovalni tlak","bar","42","42"]
["Dodatni grelec","Kapaciteta","","","kW","1.2","1.2"]