{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":7,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWS-BA3Z2"]
[]
[]
[]
[]
["","","","","","EKHWS200BA3Z2","EKHWS300BA3Z2"]
["Dodatni grelec","Kapaciteta","","","kW","3","3"]
["Mere","Enota","","Širina","mm","595","595"]
["","","Višina","Rezervoar","mm","1,195","1,645"]
["","","","Globina","mm","595","595"]
["Ohišje","Material","","","","Z epoksijem premazano plavljeno jeklo","Z epoksijem premazano plavljeno jeklo"]
["","Barva","","","","Nevtralno bela","Nevtralno bela"]
["Rezervoar","Razred energijske učinkovitosti","","","","C","C"]
["","Material","","","","Nerjavno jeklo (DIN 1,4521)","Nerjavno jeklo (DIN 1,4521)"]
["","Volumen vode","","","l","200","285"]
["Teža","Enota","","Prazno","kg","49","62"]
["Opombe","","","","","(1) - Toplotna izguba v skladu z EN12897","(1) - Toplotna izguba v skladu z EN12897"]