{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":5,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKRTR"]
[]
[]
[]
[]
["","","","","EKRTR1"]
["Funkcija regulacije","","","","Proporcionani trak"]
["Mere","Sprejemnik","Višina","mm","170"]
["","","Globina","mm","28"]
["","","Širina","mm","50"]
["","Termostat","Globina","mm","34"]
["","","Širina","mm","125"]
["","","Višina","mm","87"]
["Razpon nastavitev temperature","Gretje","Maks.","°C","37"]
["","","Min.","°C","4"]
["","Hlajenje","Maks.","°C","37"]
["","","Min.","°C","4"]
["Ura","","","","Da"]
["Teža","Sprejemnik","","g","125"]
["","Termostat","","g","210"]
["Temperatura okolice","Skladiščenje","Maks.","°F","140"]
["","","Min.","°C","-20"]
["","","Maks.","°C","60"]
["","","Min.","°F","-4"]
["","Delovanje","Min.","°C","0"]
["","","Maks.","°F","122"]
["","","Min.","°F","32"]
["","","Maks.","°C","50"]
["Maksimalni nominalni izmenični tok (pri 230 VAC)","A","","","4.0 (1)"]
["Maksimalna razdalja do sprejemnika","Zunaj","","m","približno 100m"]
["","Znotraj","","m","približno 30 m"]
["Priključek","Termostat","","","Brezžičen"]
["","Sprejemnik","","","Žičen"]
["Power supply","Faza","","","1~"]
["","Frekvenca","","Hz","50"]
["","Sprejemnik","Napetost","V","230"]
["","Termostat","Napetost","V","Baterijsko napajanje 3x AA-LRG (alkalne)"]
["Opombe","","","","(1) - 230VAC"]