{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELVH-E9W"]
[]
[]
[]
[]
["","","","","","ELVH12S23EJ9W","ELVH12S18EJ9W"]
["Ohišje","Barva","","","","Bela + Črna","Bela + Črna"]
["","Material","","","","Vnaprej premazana pločevina","Vnaprej premazana pločevina"]
["Mere","Enota","","Višina","mm","1,855","1,655"]
["","","","Širina","mm","595","595"]
["","","","Globina","mm","634","634"]
["Teža","Enota","","","kg","129","120"]
["PED","Kategorija","","","","Kategorija II","Kategorija II"]
["Raven zvočne moči","Nom.","","","dBA","44.0 (4)","44.0 (4)"]
["Raven zvočnega tlaka","Nom.","","","dBA","30.0 (4)","30.0 (4)"]
["Območje delovanja","Gretje","Stran vode","Min.","°C","15 (5)","15 (5)"]
["","","","Maks.","°C","65 (5)","65 (5)"]
["","Hlajenje","Okolje","Min.","°CDB","10 (5)","10 (5)"]
["","","Stran vode","Min.","°C","5 (5)","5 (5)"]
["","","","Maks.","°C","22 (5)","22 (5)"]
["Napajanje","Ime","","","","Glejte opombo 6","Glejte opombo 6"]
["Električni grelnik","Napajanje","","Ime","","9W","9W"]
["","","","Faza","","3~","3~"]
["","","","Napetost","V","400","400"]
["","Priporočene varovalke","","","A","20.000 (7)","20.000 (7)"]
["Opombe","","","","","(1) - Obratovalno območje je razširjeno na nižje hitrosti pretoka glede na način delovanja − glejte krivuljo ESP.","(1) - Obratovalno območje je razširjeno na nižje hitrosti pretoka glede na način delovanja − glejte krivuljo ESP."]
["","","","","","(2) - Na osnovi dT za 45 K","(2) - Na osnovi dT za 45 K"]
["","","","","","(3) - Vključno s cevmi + PHE + rezervnim grelcem, brez ekspanzijske posode","(3) - Vključno s cevmi + PHE + rezervnim grelcem, brez ekspanzijske posode"]
["","","","","","(4) - Izmerjeno s padcem tlaka 10 kPa v sistemu za gretje pri temperaturi izstopne vode 47-55 °C v prostoru s temperaturo 20 °C. DB/WB 7 °C/6°.","(4) - Izmerjeno s padcem tlaka 10 kPa v sistemu za gretje pri temperaturi izstopne vode 47-55 °C v prostoru s temperaturo 20 °C. DB/WB 7 °C/6°."]
["","","","","","(5) - Več podrobnosti preverite na risbi z obratovalnim razponom","(5) - Več podrobnosti preverite na risbi z obratovalnim razponom"]
["","","","","","(6) - 4 poli 20 A krivulja 400 V izklopilni razred C (glejte diagram ožičenja)","(6) - 4 poli 20 A krivulja 400 V izklopilni razred C (glejte diagram ožičenja)"]