{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERGA-EV"]
[]
[]
[]
[]
["","","","","","ERGA04EAV3"]
["Mere","Enota","","Višina","mm","740"]
["","","","Širina","mm","884"]
["","","","Globina","mm","388"]
["Teža","Enota","","","kg","58.5"]
["Del. doseg","Hlajenje","","Min.","°CDB","10"]
["","","","Maks.","°CDB","43"]
["Območje delovanja","Vroča voda","","Min.","°CDB","-25"]
["Del. doseg","Gosp. topla voda","","Maks.","°CDB","35"]
["Raven zvočne moči","Gretje","","Nom.","dBA","58 (1)"]
["","Hlajenje","","Nom.","dBA","61 (1)"]
["Raven zvočnega tlaka","Gretje","","Nom.","dBA","44 (1)"]
["","Hlajenje","","Nom.","dBA","48 (1)"]
["Hladilno sredstvo","Tip","","","","R-32"]
["","GWP","","","","675.0"]
["","Polnjenje","","","tCO2Eq","1.01"]
["","Polnitev","","","kg","1.50"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","6"]
["","Plin","","Zun. premer","mm","15.9"]
["Priključki napeljave","priključka","","OD","mm","18"]
["","Višinska razlika","IU - OU","Maks.","m","20.0"]
["Priključki cevne napeljave","Toplotna izolacija","","","","Tako cevi za tekočine kot za pline"]
["Napajanje","Ime","","","","V3"]
["","Faza","","","","1N~"]
["","Frekvenca","","","Hz","50"]
["","Napetost","","","V","230"]
["Tok","Priporočene varovalke","","","A","20"]
["Opombe","","","","","(1) - Hlajenje Ta 35° C - LWE 18° C (DT = 5° C); Gretje Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)"]