{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":8,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETBX16E6V / EPRA014-018DW"]
[]
[]
[]
[]
["","","","","","ETBX16EF6V / EPRA14DAW1","ETBX16EF6V / EPRA16DAW1","ETBX16EF6V / EPRA18DAW1"]
["Grelna kapaciteta","Min.","","","kW","3.70 (1)","3.96 (1)","4.40 (1)"]
["","Nom.","","","kW","5.90 (2)","9.00 (2)","9.00 (2)"]
["","Maks.","","","kW","9.75 (1)","10.44 (1)","11.60 (1)"]
["Hladilna kapaciteta","Nom.","","","kW","10.6 (3), 6.90 (4)","11.5 (3), 7.88 (4)","12.5 (3), 8.86 (4)"]
["Vhodna moč","Gretje","","Min.","kW","0.84 (5)","0.90 (5)","1.00 (5)"]
["","","","Nom.","kW","1.23 (2)","1.80 (2)","1.80 (2)"]
["","","","Maks.","kW","2.17 (5)","2.32 (5)","2.58 (5)"]
["","Hlajenje","","Nom.","kW","2.55 (3), 2.56 (4)","2.80 (3), 2.93 (4)","3.05 (3), 3.31 (4)"]
["COP","","","","","4.79 (2)","5.00 (2)","5.00 (2)"]
["EER","","","","","4.13 (3), 2.70 (4)","4.11 (3), 2.69 (4)","4.09 (3), 2.68 (4)"]
["Ogrevanje prostora","Izhod vode v povprečnem podnebju 55°C","Splošno","SCOP","","3.63","3.63","3.63"]
["","","","Razred učinkovitosti sezonskega ogrevanja prostora","","A++","A++","A++"]
["","Izhod vode v povprečnem podnebju 35°C","Splošno","SCOP","","4.81","4.81","4.81"]
["","","","Razred učinkovitosti sezonskega ogrevanja prostora","","A+++","A+++","A+++"]
["Razpon energetske učinkovitosti","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Opombe","","","","","(1) - Zmogljivost v skladu s standardom EN14511 in veljavna za toplo vodo v razponu dT = 3~8 °C pri Ta 7 °C","(1) - Zmogljivost v skladu s standardom EN14511 in veljavna za toplo vodo v razponu dT = 3~8 °C pri Ta 7 °C","(1) - Zmogljivost v skladu s standardom EN14511 in veljavna za toplo vodo v razponu dT = 3~8 °C pri Ta 7 °C"]
["","","","","","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)"]
["","","","","","(3) - Hlajenje: EW 23°C; LW 18°C; okoljski pogoji: 35°CDB","(3) - Hlajenje: EW 23°C; LW 18°C; okoljski pogoji: 35°CDB","(3) - Hlajenje: EW 23°C; LW 18°C; okoljski pogoji: 35°CDB"]
["","","","","","(4) - Hlajenje: EW 12°C; LW 7°C; okoljski pogoji: 35°CDB","(4) - Hlajenje: EW 12°C; LW 7°C; okoljski pogoji: 35°CDB","(4) - Hlajenje: EW 12°C; LW 7°C; okoljski pogoji: 35°CDB"]
["","","","","","(5) - Vhodna moč je skupna vhodna moč notranjih in zunanjih enot, vključno z obtočno črpalko; v skladu z EN14511","(5) - Vhodna moč je skupna vhodna moč notranjih in zunanjih enot, vključno z obtočno črpalko; v skladu z EN14511","(5) - Vhodna moč je skupna vhodna moč notranjih in zunanjih enot, vključno z obtočno črpalko; v skladu z EN14511"]
["","","","","","(6) - Preizkus pri Ta DB/WB 7 °C/6 °C. V skladu z EN 16147.","(6) - Preizkus pri Ta DB/WB 7 °C/6 °C. V skladu z EN 16147.","(6) - Preizkus pri Ta DB/WB 7 °C/6 °C. V skladu z EN 16147."]
["","","","","","(7) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(7) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(7) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti"]