{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETBX16E9W / EPRA014-018DW"]
[]
[]
[]
[]
["","","","","","ETBX16EF9W / EPRA14DAW1","ETBX16EF9W / EPRA16DAW1","ETBX16EF9W / EPRA18DAW1"]
["COP","","","","","4.79","5.00 (2)","5.00"]
["Ogrevanje prostora","Izhod vode v povprečnem podnebju 55°C","Splošno","Seasonal space heating eff. class","","","A++"]
["","","","ηs (Sezonska učinkovitost ogrevanja prostora)","%","","142"]
["","","","SCOP","","","3.63"]
["Cooling capacity","Nom.","","","kW","","11.5 (3), 7.88 (4)"]
["EER","","","","","4.13, 2.70","4.11 (3), 2.69 (4)","4.09, 2.68"]
["Zmogljivost gretja","Nom.","","","kW","","9.00 (2)"]
["","Min.","","","kW","","3.96 (1)"]
["","Maks.","","","kW","","10.44 (1)"]
["Vhodna moč","Hlajenje","","Nom.","kW","","2.80 (3), 2.93 (4)"]
["","Gretje","","Maks.","kW","","2.32 (5)"]
["","","","Min.","kW","","0.90 (5)"]
["","","","Nom.","kW","","1.80 (2)"]
["Opombe","","","","","(1) - Zmogljivost v skladu s standardom EN14511 in veljavna za toplo vodo v razponu dT = 3~8 °C pri Ta 7 °C","(1) - Zmogljivost v skladu s standardom EN14511 in veljavna za toplo vodo v razponu dT = 3~8 °C pri Ta 7 °C","(1) - Zmogljivost v skladu s standardom EN14511 in veljavna za toplo vodo v razponu dT = 3~8 °C pri Ta 7 °C"]
["","","","","","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)"]
["","","","","","(3) - Hlajenje: EW 23°C; LW 18°C; okoljski pogoji: 35°CDB","(3) - Hlajenje: EW 23°C; LW 18°C; okoljski pogoji: 35°CDB","(3) - Hlajenje: EW 23°C; LW 18°C; okoljski pogoji: 35°CDB"]
["","","","","","(4) - Hlajenje: EW 12°C; LW 7°C; okoljski pogoji: 35°CDB","(4) - Hlajenje: EW 12°C; LW 7°C; okoljski pogoji: 35°CDB","(4) - Hlajenje: EW 12°C; LW 7°C; okoljski pogoji: 35°CDB"]
["","","","","","(5) - Vhodna moč je skupna vhodna moč notranjih in zunanjih enot, vključno z obtočno črpalko; v skladu z EN14511","(5) - Vhodna moč je skupna vhodna moč notranjih in zunanjih enot, vključno z obtočno črpalko; v skladu z EN14511","(5) - Vhodna moč je skupna vhodna moč notranjih in zunanjih enot, vključno z obtočno črpalko; v skladu z EN14511"]
["","","","","","(6) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(6) - Preizkus pri Ta DB/WB 7 °C/6 °C. V skladu z EN 16147.","(6) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti"]
["","","","","","","(7) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti"]
["Grelna kapaciteta","Min.","","","kW","3.70","","4.40"]
["","Nom.","","","kW","5.90","","9.00"]
["","Maks.","","","kW","9.75","","11.60"]
["Hladilna kapaciteta","Nom.","","","kW","10.6, 6.90","","12.5, 8.86"]
["Vhodna moč","Gretje","","Min.","kW","0.84","","1.00"]
["","","","Nom.","kW","1.23","","1.80"]
["","","","Maks.","kW","2.17","","2.58"]
["","Hlajenje","","Nom.","kW","2.55, 2.56","","3.05, 3.31"]
["Ogrevanje prostora","Izhod vode v povprečnem podnebju 55°C","Splošno","SCOP","","3.63","","3.63"]
["","","","Razred učinkovitosti sezonskega ogrevanja prostora","","A++","","A++"]
["","Izhod vode v povprečnem podnebju 35°C","Splošno","SCOP","","4.81","","4.81"]
["","","","Razred učinkovitosti sezonskega ogrevanja prostora","","A+++","","A+++"]